----------------------------------------------------------------------
Patch name: Cosimulation support
Date: 25 Jan 2006
Status: Cosimulation not working yet.

Detailed description:

The cosimulation feature doesn't work since Bochs 2.0 release (or may be 
even earlier).

According to my opinion it should be redefined and implemented in totally
different way; for example two Bochs simulators compiled with cosimulation
could connect through pipe or TCP/IP and run together comparing the arch 
automatically state or on demand.
Let's assume we have dynamic translation support in Bochs, so we could
compile it with cosimulation and run two Bochs binaries compiled with 
dynamic translation and without and compare between them automatically 
to assure emulation correctness. The same for any other performance feature. 
This cosimulation approach should reach the same goals but do it in same 
strange way ...

OK, I assume the patch could be automatically applied to Bochs 2.2.6 release
without any conflicts, but do not think it will work or even compile !
The patch is more FYI s.t. you will be able to look on some cosimulation
implementation during developing a new one ;)

And just to be sure ... 
I marked the patch root in CVS with tag bochs-cosimulation-patch-root
so you always could find some Bochs version to apply it ;)

Patch was created with:
  cvs diff -ubBwNp

Instructions:
  To patch, apply patch to main bochs directory:
    > patch -p1 < cosim-patch
  I skipped automatically generated files from this patch to 
  reduce its absolute size.
  To regenerate configure file:
    > autoconf configure.in > configure
  To regenerate lexer.c, parser.c and parser.h
    > cd bx_debug; rm -f lexer.c parser.c parser.h; make
----------------------------------------------------------------------

diff -uBbwNpr bochs-nocosim/bochs.h bochs/bochs.h
--- bochs-nocosim/bochs.h	2006-01-25 22:50:48.078125000 +0200
+++ bochs/bochs.h	2006-01-20 21:12:03.000000000 +0200
@@ -118,6 +118,37 @@ void bx_reset_options (void);
 // needed.
 //
 
+#if ((BX_DEBUGGER == 1) && (BX_NUM_SIMULATORS >= 2))
+
+// =-=-=-=-=-=-=- Redirected to cosimulation debugger -=-=-=-=-=-=-=
+#define DEV_vga_mem_read(addr)       bx_dbg_ucmem_read(addr)
+#define DEV_vga_mem_write(addr, val) bx_dbg_ucmem_write(addr, val)
+
+#define BX_INP(addr, len)           bx_dbg_inp(addr, len)
+#define BX_OUTP(addr, val, len)     bx_dbg_outp(addr, val, len)
+#define BX_HRQ                      (bx_pc_system.HRQ)
+#define BX_RAISE_HLDA()             bx_dbg_raise_HLDA()
+#define BX_TICK1()
+#define BX_INTR                     bx_pc_system.INTR
+#define BX_SET_INTR(b)              bx_dbg_set_INTR(b)
+#if BX_SIM_ID == 0
+#  define BX_CPU_C                  bx_cpu0_c
+#  define BX_CPU                    bx_cpu0
+#  define BX_MEM_C                  bx_mem0_c
+#  define BX_MEM                    bx_mem0
+#else
+#  define BX_CPU_C                  bx_cpu1_c
+#  define BX_CPU                    bx_cpu1
+#  define BX_MEM_C                  bx_mem1_c
+#  define BX_MEM                    bx_mem1
+#endif
+#define BX_SET_ENABLE_A20(enabled)  bx_dbg_async_pin_request(BX_DBG_ASYNC_PENDING_A20, \
+                                      enabled)
+#define BX_GET_ENABLE_A20()         bx_pc_system.get_enable_a20()
+#error FIXME: cosim mode not fixed yet
+
+#else
+
 // =-=-=-=-=-=-=- Normal optimized use -=-=-=-=-=-=-=-=-=-=-=-=-=-=
 // some pc_systems functions just redirect to the IO devices so optimize
 // by eliminating call here
@@ -153,6 +184,8 @@ void bx_reset_options (void);
 #define BX_SET_ENABLE_A20(enabled)  bx_pc_system.set_enable_a20(enabled)
 #define BX_GET_ENABLE_A20()         bx_pc_system.get_enable_a20()
 
+#endif
+
 #if BX_SUPPORT_A20
 #  define A20ADDR(x)                ((x) & bx_pc_system.a20_mask)
 #else
@@ -176,6 +210,21 @@ void bx_reset_options (void);
 #if BX_DEBUGGER
 #  define BX_DBG_ASYNC_INTR bx_guard.async.irq
 #  define BX_DBG_ASYNC_DMA  bx_guard.async.dma
+#if (BX_NUM_SIMULATORS > 1)
+// for multiple simulators, we always need this info, since we're
+// going to replay it.
+#  define BX_DBG_DMA_REPORT(addr, len, what, val) \
+        bx_dbg_dma_report(addr, len, what, val)
+#  define BX_DBG_IAC_REPORT(vector, irq) \
+        bx_dbg_iac_report(vector, irq)
+#  define BX_DBG_A20_REPORT(val) \
+        bx_dbg_a20_report(val)
+#  define BX_DBG_IO_REPORT(addr, size, op, val) \
+        bx_dbg_io_report(addr, size, op, val)
+#  define BX_DBG_UCMEM_REPORT(addr, size, op, val)
+#else
+// for a single simulator debug environment, we can optimize a little
+// by conditionally calling, as per requested.
 
 #  define BX_DBG_DMA_REPORT(addr, len, what, val) \
         if (bx_guard.report.dma) bx_dbg_dma_report(addr, len, what, val)
@@ -187,6 +236,8 @@ void bx_reset_options (void);
         if (bx_guard.report.io) bx_dbg_io_report(addr, size, op, val)
 #  define BX_DBG_UCMEM_REPORT(addr, size, op, val) \
         if (bx_guard.report.ucmem) bx_dbg_ucmem_report(addr, size, op, val)
+#endif  // #if (BX_NUM_SIMULATORS > 1)
+
 #else  // #if BX_DEBUGGER
 // debugger not compiled in, use empty stubs
 #  define BX_DBG_ASYNC_INTR 1
diff -uBbwNpr bochs-nocosim/bx_debug/Makefile.in bochs/bx_debug/Makefile.in
--- bochs-nocosim/bx_debug/Makefile.in	2006-01-25 22:46:16.062500000 +0200
+++ bochs/bx_debug/Makefile.in	2006-01-24 21:03:53.000000000 +0200
@@ -56,6 +56,7 @@ YACC   = yacc
 BX_OBJS = \
   dbg_main.o \
   symbols.o \
+  cosim.o \
   linux.o \
 
 BX_PARSER_OBJS = \
@@ -147,3 +148,17 @@ symbols.o: symbols.@CPP_SUFFIX@ ../bochs
   ../cpu/xmm.h ../memory/memory.h ../pc_system.h ../plugin.h \
   ../extplugin.h ../ltdl.h ../gui/gui.h ../gui/textconfig.h \
   ../gui/keymap.h ../instrument/stubs/instrument.h
+cosim.o: cosim.@CPP_SUFFIX@ ../bochs.h ../config.h ../osdep.h ../bx_debug/debug.h \
+  ../bxversion.h ../gui/siminterface.h ../cpu/cpu.h ../cpu/lazy_flags.h \
+  ../cpu/hostasm.h ../cpu/icache.h ../cpu/apic.h ../cpu/i387.h \
+  ../fpu/softfloat.h ../fpu/tag_w.h ../fpu/status_w.h ../fpu/control_w.h \
+  ../cpu/xmm.h ../memory/memory.h ../pc_system.h ../plugin.h \
+  ../extplugin.h ../ltdl.h ../gui/gui.h ../gui/textconfig.h \
+  ../gui/keymap.h ../instrument/stubs/instrument.h
+sim2.o: sim2.@CPP_SUFFIX@ ../bochs.h ../config.h ../osdep.h ../bx_debug/debug.h \
+  ../bxversion.h ../gui/siminterface.h ../cpu/cpu.h ../cpu/lazy_flags.h \
+  ../cpu/hostasm.h ../cpu/icache.h ../cpu/apic.h ../cpu/i387.h \
+  ../fpu/softfloat.h ../fpu/tag_w.h ../fpu/status_w.h ../fpu/control_w.h \
+  ../cpu/xmm.h ../memory/memory.h ../pc_system.h ../plugin.h \
+  ../extplugin.h ../ltdl.h ../gui/gui.h ../gui/textconfig.h \
+  ../gui/keymap.h ../instrument/stubs/instrument.h
diff -uBbwNpr bochs-nocosim/bx_debug/cosim.cc bochs/bx_debug/cosim.cc
--- bochs-nocosim/bx_debug/cosim.cc	1970-01-01 02:00:00.000000000 +0200
+++ bochs/bx_debug/cosim.cc	2006-01-15 19:55:25.000000000 +0200
@@ -0,0 +1,979 @@
+/////////////////////////////////////////////////////////////////////////
+// $Id: patch.cosimulation,v 1.2 2006-01-25 22:30:07 sshwarts Exp $
+/////////////////////////////////////////////////////////////////////////
+//
+//  Copyright (C) 2001  MandrakeSoft S.A.
+//
+//    MandrakeSoft S.A.
+//    43, rue d'Aboukir
+//    75002 Paris - France
+//    http://www.linux-mandrake.com/
+//    http://www.mandrakesoft.com/
+//
+//  This library is free software; you can redistribute it and/or
+//  modify it under the terms of the GNU Lesser General Public
+//  License as published by the Free Software Foundation; either
+//  version 2 of the License, or (at your option) any later version.
+//
+//  This library is distributed in the hope that it will be useful,
+//  but WITHOUT ANY WARRANTY; without even the implied warranty of
+//  MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
+//  Lesser General Public License for more details.
+//
+//  You should have received a copy of the GNU Lesser General Public
+//  License along with this library; if not, write to the Free Software
+//  Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA  02111-1307 USA
+//
+
+#include "bochs.h"
+
+#if BX_NUM_SIMULATORS >= 2
+
+unsigned bx_dbg_cosimulateN(bx_dbg_icount_t count)
+{
+  // execute both master & slave for count instructions,
+  // handling asynchronous events, etc.
+  // returns 0 = didn't get through all count instructions
+  //             either a guard was hit, or a divergence occurred
+  //         1 = got through all count instructions
+
+  unsigned master, slave;
+  bx_dbg_icount_t master_icount, slave_icount;
+  bx_bool bail_out = 0;
+  unsigned ret = 0;
+  bx_bool save_INTR;
+  bx_bool pre_A20, post_A20;
+  unsigned async_head;
+  bx_dbg_icount_t async_icount, curr_icount;
+
+  if (count == 0) {
+    dbg_printf ( "Error: cosimulateN: count=0\n");
+    bx_dbg_exit(1);
+  }
+
+  bx_guard.guard_for |= BX_DBG_GUARD_ICOUNT;  // stop at icount
+  bx_guard.guard_for &= ~BX_DBG_GUARD_CTRL_C; // ignore Ctrl-C
+
+one_time_slice:
+  // take minimum of requested count and maximum count quantum
+  if (count > bx_debugger.icount_quantum)
+    bx_guard.icount = bx_debugger.icount_quantum;
+  else
+    bx_guard.icount = count;
+
+  // for now, assume...
+  master = bx_debugger.master;
+  slave  = bx_debugger.slave;
+
+  // run master simulator
+  bx_debugger.master_slave_mode = BX_DBG_MASTER_MODE;
+  if (bx_guard.interrupt_requested) {
+    bail_out = 1;
+    dbg_printf ("ctrlc typed\n");
+  }
+  bx_guard_found[master].guard_found = 0;
+  bx_guard_found[master].icount = 0;
+  if (doit) dbg_printf ("requesting run of master for %u\n",
+    (unsigned) bx_guard.icount);
+  // save A20 value before master run
+  pre_A20 = bx_pc_system.get_enable_a20();
+
+  BX_MEM(master)->cpu_loop(-1);
+  post_A20  = bx_pc_system.get_enable_a20(); // A20 after master run
+  master_icount = bx_guard_found[master].icount;
+  slave_icount = 0;
+  if (master_icount)
+    bx_pc_system.tickn(master_icount);
+  save_INTR = bx_pc_system.INTR; // value after master run
+  bx_pc_system.INTR = 0; // in case slave uses directly
+  // Change A20 for slave run to model what it was at beginning of
+  // master run, only if it needs to be changed.
+  if (pre_A20 != post_A20) {
+    bx_pc_system.set_enable_a20(pre_A20);
+    if (BX_MEM(slave)->set_A20)
+      BX_MEM(slave)->set_A20(pre_A20);
+    }
+
+  // if guard was anything except for icount, we should terminate
+  // after synchronizing slave to master
+  if (bx_guard_found[master].guard_found & ~BX_DBG_GUARD_ICOUNT)
+    bail_out = 1;
+
+  // Synchronize slave to master.  Account for Ctrl-C's typed during execution of
+  // slave.
+  bx_debugger.master_slave_mode = BX_DBG_SLAVE_MODE;
+  do {
+    // run slave for remaining instructions to catch up to master
+    curr_icount = master_icount - slave_icount;
+    if (bx_debugger.async_journal.size) {
+      // If there were asynchronous events which occurred while the
+      // master was running, have to run the slave up to each of these
+      // points individually, and force it to take them on exactly the
+      // same boundaries.
+      async_head   = bx_debugger.async_journal.head;
+      async_icount = bx_debugger.async_journal.element[async_head].icount;
+      curr_icount  = async_icount;  // only run to next async event
+      }
+    else {
+      async_head   = 0; // keep compiler happy
+      async_icount = 0; // keep compiler happy
+      }
+
+    bx_guard_found[slave].guard_found = 0;
+    bx_guard_found[slave].icount = 0;
+    bx_guard.icount = curr_icount;
+
+    if (curr_icount) {
+      // Async event may be before completion of any instructions,
+      // for example taking of interrupt.
+      if (doit) dbg_printf ( "requesting run of slave for %u\n",
+        (unsigned) bx_guard.icount);
+      if (bx_debugger.fast_forward_mode) {
+        bx_guard_found[slave].icount = curr_icount;
+        bx_guard_found[slave].guard_found = BX_DBG_GUARD_ICOUNT;
+      } else {
+        BX_MEM(slave)->cpu_loop(-1);
+      }
+    }
+    slave_icount += bx_guard_found[slave].icount;
+    if (bx_guard_found[slave].guard_found & ~BX_DBG_GUARD_ICOUNT) {
+      bail_out = 1;
+      // If user type Ctrl-C we're done after synchronizing.  If not,
+      // then we have reached a true guard, and it's time to bail.
+      if (bx_guard_found[slave].guard_found &
+          ~(BX_DBG_GUARD_ICOUNT | BX_DBG_GUARD_CTRL_C))
+        break;
+    }
+    if (bx_debugger.async_journal.size) {
+      // sanity check: slave should be at async point
+      if (bx_guard_found[slave].icount != async_icount) {
+        dbg_printf ( "Error: comsimulateN: async: slave not at sync point.\n");
+        bx_dbg_exit(1);
+      }
+      switch (bx_debugger.async_journal.element[async_head].what) {
+        case BX_DBG_ASYNC_JOURNAL_IAC:
+         if (!bx_debugger.fast_forward_mode) {
+            if (doit)
+              dbg_printf ("slave: forcing interrupt %u\n",
+                bx_debugger.async_journal.element[async_head].u.iac.val);
+
+            BX_MEM(slave)->dbg_force_interrupt(
+              bx_debugger.async_journal.element[async_head].u.iac.val);
+          }
+          break;
+        case BX_DBG_ASYNC_JOURNAL_A20:
+          bx_pc_system.set_enable_a20(
+            bx_debugger.async_journal.element[async_head].u.a20.val);
+          if (BX_MEM(slave)->set_A20)
+            BX_MEM(slave)->set_A20(
+              bx_debugger.async_journal.element[async_head].u.a20.val);
+          break;
+        case BX_DBG_ASYNC_JOURNAL_NMI:
+        case BX_DBG_ASYNC_JOURNAL_RESET:
+        default:
+          dbg_printf ( "Error: cosimulateN: unimplemented async event.\n");
+      }
+      // async event processed, dequeue it
+      bx_debugger.async_journal.size--;
+      bx_debugger.async_journal.head++;
+    }
+  } while (slave_icount < master_icount);
+
+  bx_pc_system.INTR = save_INTR; // restore INTR to value after master run
+
+  // At this point, both simulators should be at the same point.  Either
+  // they have finished executing for the desired count, or at least for
+  // a time quantum.  Check to see if the environments are in sync.
+  int iaddr_res;
+  if (!bx_debugger.fast_forward_mode) {
+    if (bx_debugger.compare_at_sync.iaddr && (iaddr_res = bx_dbg_compare_sim_iaddr())) {
+      if (iaddr_res == 1)
+        bail_out = 1;
+    } else if (bx_debugger.compare_at_sync.cpu && bx_dbg_compare_sim_cpu())
+      bail_out = 1;
+    else if (bx_debugger.compare_at_sync.memory && bx_dbg_compare_sim_memory())
+      bail_out = 1;
+  }
+
+  if (bail_out) {
+#ifdef DEBUGGER_ERROR
+    extern void DEBUGGER_ERROR(void);
+    DEBUGGER_ERROR();
+#endif
+
+    ret = 0; // didn't complete, stopped
+  }
+  else {
+    count -= master_icount;
+    // last icount known to be in sync
+    bx_debugger.last_sync_icount += master_icount;
+    if (count)
+      goto one_time_slice;
+    ret = 1; // completed OK
+  }
+
+  bx_guard.guard_for &= ~BX_DBG_GUARD_ICOUNT;
+  return(ret);
+}
+
+int bx_dbg_compare_sim_iaddr(void)
+{
+  // returns 0 = same, 1 = different, 2 = false diff
+  if (BX_CPU(dbg_cpu)->guard_found.laddr != bx_guard_found[1].laddr) {
+
+#ifdef FALSE_DIFF_DETECT
+    extern int FALSE_DIFF_DETECT();
+    if (FALSE_DIFF_DETECT())
+      return 2;
+#endif
+
+    dbg_printf (
+#if BX_DBG_ICOUNT_SIZE == 32
+      "*** Iaddr divergence ***: last know synchronized icount was %lu\n",
+      (unsigned long) bx_debugger.last_sync_icount
+#else  // BX_DBG_ICOUNT_SIZE == 64
+      "*** Iaddr divergence ***: last know synchronized icount was %Lu\n",
+      (unsigned long long) bx_debugger.last_sync_icount
+#endif
+      );
+
+//    dbg_printf ( "Divergence: sim[0].laddr=%x, sim[1].laddr=%x\n",
+//      (unsigned) BX_CPU(dbg_cpu)->guard_found.laddr,
+//      (unsigned) bx_guard_found[1].laddr);
+    return(1); // different
+  }
+  return(0); // same
+}
+
+bx_bool bx_dbg_compare_sim_cpu(void)
+{
+  // (mch) Get cpu structures from both simulators
+
+  // Compare the structures (except the descriptor parts of the
+  // segment registers
+  bx_dbg_cpu_t regs[2];
+
+  BX_MEM(0)->dbg_get_cpu(regs + 0);
+  BX_MEM(1)->dbg_get_cpu(regs + 1);
+
+  bx_bool ret = 0;
+  bx_bool warn = 0;
+
+  // (mch) Yes I know these are macros. The would have been
+  // inner functions if g++ had supported it.
+#define TEST_REG(reg, reg_name) \
+  do { \
+    if (regs[0].reg != regs[1].reg) { \
+      printf("COSIM ERROR: [%s] %s: 0x%08x  %s: 0x%08x\n", reg_name, SIM_NAME0, regs[0].reg, SIM_NAME1_STR, regs[1].reg); \
+      ret = 1; \
+    } \
+  } while(0)
+
+#define TEST_REG_WARN(reg, reg_name, mask) \
+  do { \
+    if ((regs[0].reg & mask) != (regs[1].reg & mask)) { \
+      printf("COSIM WARNING: [%s] %s: 0x%08x  %s: 0x%08x\n", reg_name, SIM_NAME0, (regs[0].reg & mask), SIM_NAME1_STR, (regs[1].reg & mask)); \
+      warn = 1; \
+    } \
+  } while(0)
+
+  TEST_REG(eax, "eax");
+  TEST_REG(ebx, "ebx");
+  TEST_REG(ecx, "ecx");
+  TEST_REG(edx, "edx");
+  TEST_REG(ebp, "ebp");
+  TEST_REG(esi, "esi");
+  TEST_REG(edi, "edi");
+  TEST_REG(esp, "esp");
+        TEST_REG_WARN(eflags, "eflags & CF", 0x1);
+#define EFLAGS_MASK (~((1 << 11) | (1 << 7) | (1 << 6) | (1 << 4) | (1 << 2) | (1 << 0)))
+  regs[0].eflags &= EFLAGS_MASK;
+  regs[1].eflags &= EFLAGS_MASK;
+  TEST_REG(eflags, "eflags");
+  TEST_REG(eip, "eip");
+
+#define TEST_SEG_REG(reg, reg_name) \
+  do { \
+    if (regs[0].reg.sel != regs[1].reg.sel || regs[0].reg.valid != regs[1].reg.valid) { \
+      printf("COSIM ERROR: [%s] %s: 0x%04x (%d)  %s: 0x%04x (%d)\n", reg_name, SIM_NAME0, regs[0].reg.sel, regs[0].reg.valid, SIM_NAME1_STR, regs[1].reg.sel, regs[1].reg.valid); \
+      ret = 1; \
+    } \
+  } while(0)
+
+  TEST_SEG_REG(cs, "cs");
+  TEST_SEG_REG(ss, "ss");
+  TEST_SEG_REG(ds, "ds");
+  TEST_SEG_REG(es, "es");
+  TEST_SEG_REG(fs, "fs");
+  TEST_SEG_REG(gs, "gs");
+  TEST_SEG_REG(ldtr, "ldtr");
+  TEST_SEG_REG(tr, "tr");
+
+  if (regs[0].gdtr.base != regs[1].gdtr.base || regs[0].gdtr.limit != regs[1].gdtr.limit) {
+    printf("COSIM ERROR: [gdtr] %s: 0x%08x:0x%04x  %s 0x%08x:0x%04x\n",
+           SIM_NAME0, regs[0].gdtr.base, regs[0].gdtr.limit, SIM_NAME1_STR, regs[1].gdtr.base, regs[1].gdtr.limit);
+    ret = 1;
+  }
+  if (regs[0].idtr.base != regs[1].idtr.base || regs[0].idtr.limit != regs[1].idtr.limit) {
+    printf("COSIM ERROR: [idtr] %s: 0x%08x:0x%04x  %s 0x%08x:0x%04x\n",
+           SIM_NAME0, regs[0].idtr.base, regs[0].idtr.limit, SIM_NAME1_STR, regs[1].idtr.base, regs[1].idtr.limit);
+    ret = 1;
+  }
+
+  // drX ignored
+  // trX ignored
+
+  TEST_REG(cr0, "cr0");
+  TEST_REG(cr1, "cr1");
+  TEST_REG(cr2, "cr2");
+  TEST_REG(cr3, "cr3");
+  TEST_REG(cr4, "cr4");
+
+  if (regs[0].inhibit_mask != regs[1].inhibit_mask) {
+    printf("COSIM ERROR [inhibit_mask] %s: %d  %s: %d\n",
+           SIM_NAME0, regs[0].inhibit_mask, SIM_NAME1_STR, regs[1].inhibit_mask);
+    ret = 1;
+  }
+
+  if (ret) {
+    dbg_printf (
+#if BX_DBG_ICOUNT_SIZE == 32
+      "*** CPU divergence ***: last know synchronized icount was %lu\n",
+      (unsigned long) bx_debugger.last_sync_icount
+#else  // BX_DBG_ICOUNT_SIZE == 64
+      "*** CPU divergence ***: last know synchronized icount was %Lu\n",
+      (unsigned long long) bx_debugger.last_sync_icount
+#endif
+      );
+  } else if (warn) {
+    dbg_printf (
+#if BX_DBG_ICOUNT_SIZE == 32
+      "=== CPU divergence ===: last know synchronized icount was %lu\n",
+      (unsigned long) bx_debugger.last_sync_icount
+#else  // BX_DBG_ICOUNT_SIZE == 64
+      "=== CPU divergence ===: last know synchronized icount was %Lu\n",
+      (unsigned long long) bx_debugger.last_sync_icount
+#endif
+      );
+#ifdef DEBUGGER_ERROR
+    extern void DEBUGGER_ERROR(void);
+    DEBUGGER_ERROR();
+#endif
+  }
+
+  return ret;
+}
+
+void clear_dirty_bits (void)
+{
+  int num_pages = bx_options.memory.Osize->get () * 1024 / 4;
+  for (int i = 0; i < num_pages; i++) {
+    BX_MEM(0)->dbg_dirty_pages[i] = 0;
+    BX_MEM(1)->dbg_dirty_pages[i] = 0;
+  }
+}
+
+bx_bool always_check_page[128 * 1024 / 4];
+
+void bx_dbg_always_check(Bit32u page_start, bx_bool on)
+{
+  always_check_page[page_start / (4 * 1024)] = on;
+  printf("Forced check on page %08x %s\n",
+         page_start, on ? "enabled" : "disabled");
+}
+
+bx_bool bx_dbg_compare_sim_memory(void)
+{
+  bx_bool ret = 0;
+  int num_pages = bx_options.memory.Osize->get () * 1024 / 4;
+
+  for (int i = 0; i < num_pages; i++) {
+    bx_bool sim0_dirty = BX_MEM(0)->dbg_dirty_pages[i];
+    bx_bool sim1_dirty = BX_MEM(1)->dbg_dirty_pages[i];
+    Bit32u page_start = i * 1024 * 4;
+
+    if ((sim0_dirty != sim1_dirty) || sim0_dirty || always_check_page[i]) {
+      // Page has been written, compare
+      // (mch) I'm quite aware of how hackish this is. I don't care.
+      extern Bit8u* SIM1_GET_PHYS_PTR(Bit32u page_start);
+      Bit8u* sim0_page_vec = bx_mem0.vector + page_start;
+      Bit8u* sim1_page_vec = SIM1_GET_PHYS_PTR(page_start);
+
+      if (memcmp(sim0_page_vec, sim1_page_vec, 1024 * 4)) {
+        printf("COSIM ERROR  Physical page %08x differs in content\n", page_start);
+        for (int j = 0; j < 1024 * 4; j++) {
+          if (sim0_page_vec[j] != sim1_page_vec[j]) {
+            printf("%08x   %s: %02x  %s: %02x\n",
+                   page_start+j, SIM_NAME0, sim0_page_vec[j], SIM_NAME1_STR, sim1_page_vec[j]);
+          }
+        }
+        ret = 1;
+      }
+    }
+  }
+
+  if (ret) {
+    dbg_printf (
+#if BX_DBG_ICOUNT_SIZE == 32
+      "*** Memory divergence ***: last know synchronized icount was %lu\n",
+      (unsigned long) bx_debugger.last_sync_icount
+#else  // BX_DBG_ICOUNT_SIZE == 64
+      "*** Memory divergence ***: last know synchronized icount was %Lu\n",
+      (unsigned long long) bx_debugger.last_sync_icount
+#endif
+      );
+  }
+
+  clear_dirty_bits();
+
+  return ret;
+}
+
+void bx_dbg_journal_a20_event(unsigned val)
+{
+  unsigned tail, master;
+
+  if (bx_debugger.master_slave_mode == BX_DBG_SLAVE_MODE ) {
+    dbg_printf ( "Error: a20_report: in slave mode.\n");
+    bx_dbg_exit(1);
+  }
+
+  // Master simulator mode
+  if (bx_debugger.async_journal.size >= BX_DBG_ASYNC_JOURNAL_SIZE) {
+    dbg_printf ( "Error: async journal full.\n");
+    bx_dbg_exit(1);
+  }
+
+  if (bx_debugger.async_journal.size == 0) {
+    // start off point head & tail at same element
+    bx_debugger.async_journal.head = 0;
+    tail = bx_debugger.async_journal.tail = 0;
+  }
+  else {
+    tail = bx_debugger.async_journal.tail + 1;
+  }
+  if (tail >= BX_DBG_ASYNC_JOURNAL_SIZE) {
+    dbg_printf ( "Error: a20_report: journal wrapped.\n");
+    bx_dbg_exit(0);
+  }
+
+  master = bx_debugger.master;
+  bx_debugger.async_journal.element[tail].what = BX_DBG_ASYNC_JOURNAL_A20;
+  bx_debugger.async_journal.element[tail].icount = bx_guard_found[master].icount;
+  bx_debugger.async_journal.element[tail].u.a20.val = val;
+
+  if (bx_debugger.async_journal.size)
+    bx_debugger.async_journal.tail++;
+  bx_debugger.async_journal.size++;
+}
+
+Bit8u bx_dbg_ucmem_read(Bit32u addr)
+{
+  Bit8u value;
+  unsigned head, tail;
+
+  if ( bx_debugger.master_slave_mode == BX_DBG_MASTER_MODE ) {
+    if (!bx_debugger.fast_forward_mode) {
+      if (bx_debugger.UCmem_journal.size >= BX_DBG_UCMEM_JOURNAL_SIZE) {
+        dbg_printf ( "dbg_ucmem_read: journal full.\n");
+        bx_dbg_exit(0);
+      }
+
+      if (bx_debugger.UCmem_journal.size == 0) {
+        // start off point head & tail at same element
+        bx_debugger.UCmem_journal.head = 0;
+        tail = bx_debugger.UCmem_journal.tail = 0;
+      }
+      else {
+        tail = bx_debugger.UCmem_journal.tail + 1;
+      }
+      if (tail >= BX_DBG_UCMEM_JOURNAL_SIZE) {
+        dbg_printf ( "dbg_ucmem_read: journal wrapped.\n");
+        bx_dbg_exit(0);
+      }
+
+      value = DEV_vga_mem_read(addr);
+      bx_dbg_ucmem_report(addr, 1, BX_READ, value);
+      bx_debugger.UCmem_journal.element[tail].op    = BX_READ;
+      bx_debugger.UCmem_journal.element[tail].len   = 1;
+      bx_debugger.UCmem_journal.element[tail].addr  = addr;
+      bx_debugger.UCmem_journal.element[tail].value = value;
+      if (bx_debugger.UCmem_journal.size)
+        bx_debugger.UCmem_journal.tail++;
+      bx_debugger.UCmem_journal.size++;
+
+      if (doit)
+        dbg_printf ( "MASTER UCR: head:%u tail%u size:%u\n",
+          bx_debugger.UCmem_journal.head,
+          bx_debugger.UCmem_journal.tail,
+          bx_debugger.UCmem_journal.size);
+
+      return(value);
+    } else {
+      value = DEV_vga_mem_read(addr);
+      return(value);
+    }
+  }
+  else {
+    if (bx_debugger.UCmem_journal.size == 0) {
+      dbg_printf ( "Error: ucmem_read: journal empty.\n");
+      return(0xff);
+    }
+    head = bx_debugger.UCmem_journal.head;
+    value = bx_debugger.UCmem_journal.element[head].value;
+
+    if ((bx_debugger.UCmem_journal.element[head].op != BX_READ) ||
+        (bx_debugger.UCmem_journal.element[head].len != 1) ||
+        (bx_debugger.UCmem_journal.element[head].addr != addr))
+    {
+      dbg_printf ( "Error: ucmem_read: out of sync with journal.\n");
+      dbg_printf ( "Error: master: op=%1s len=%u addr=0x%x val=0x%x\n",
+        (bx_debugger.UCmem_journal.element[head].op==BX_READ) ? "W" : "R",
+        (unsigned) bx_debugger.UCmem_journal.element[head].len,
+        (unsigned) bx_debugger.UCmem_journal.element[head].addr,
+        (unsigned) bx_debugger.UCmem_journal.element[head].value);
+      dbg_printf ( "Error: slave:  op=W len=%u addr=0x%x val=0x%x\n",
+        (unsigned) 1, (unsigned) addr, (unsigned) value);
+      return(0xff);
+    }
+    // slave UCmem op in sync with journaled master op, delete this entry
+    bx_debugger.UCmem_journal.head++;
+    bx_debugger.UCmem_journal.size--;
+    return(value);
+  }
+}
+
+void bx_dbg_ucmem_write(Bit32u addr, Bit8u value)
+{
+  unsigned tail, head;
+
+  if ( bx_debugger.master_slave_mode == BX_DBG_MASTER_MODE ) {
+    if (!bx_debugger.fast_forward_mode) {
+      if (bx_debugger.UCmem_journal.size >= BX_DBG_UCMEM_JOURNAL_SIZE) {
+        dbg_printf ( "dbg_ucmem_write: journal full.\n");
+        bx_dbg_exit(0);
+      }
+
+      if (bx_debugger.UCmem_journal.size == 0) {
+        // start off point head & tail at same element
+        bx_debugger.UCmem_journal.head = 0;
+        tail = bx_debugger.UCmem_journal.tail = 0;
+      }
+      else {
+        tail = bx_debugger.UCmem_journal.tail + 1;
+      }
+      if (tail >= BX_DBG_UCMEM_JOURNAL_SIZE) {
+        dbg_printf ( "dbg_ucmem_write: journal wrapped.\n");
+        bx_dbg_exit(0);
+      }
+
+      bx_debugger.UCmem_journal.element[tail].op    = BX_WRITE;
+      bx_debugger.UCmem_journal.element[tail].len   = 1;
+      bx_debugger.UCmem_journal.element[tail].addr  = addr;
+      bx_debugger.UCmem_journal.element[tail].value = value;
+
+      if (bx_debugger.UCmem_journal.size)
+        bx_debugger.UCmem_journal.tail++;
+      bx_debugger.UCmem_journal.size++;
+      DEV_vga_mem_write(addr, value);
+      bx_dbg_ucmem_report(addr, 1, BX_WRITE, value);
+    } else {
+      DEV_vga_mem_write(addr, value);
+    }
+  }
+  else {
+    if (bx_debugger.UCmem_journal.size == 0) {
+      dbg_printf ( "Error: ucmem_write: journal empty.\n");
+      return;
+    }
+    head = bx_debugger.UCmem_journal.head;
+
+    if ((bx_debugger.UCmem_journal.element[head].op != BX_WRITE) ||
+        (bx_debugger.UCmem_journal.element[head].len != 1) ||
+        (bx_debugger.UCmem_journal.element[head].addr != addr) ||
+        (bx_debugger.UCmem_journal.element[head].value != value) )
+    {
+      dbg_printf ( "Error: ucmem_write: out of sync with journal.\n");
+      dbg_printf ( "Error: master: op=%1s len=%u addr=0x%x val=0x%x\n",
+        (bx_debugger.UCmem_journal.element[head].op==BX_WRITE) ? "W" : "R",
+        (unsigned) bx_debugger.UCmem_journal.element[head].len,
+        (unsigned) bx_debugger.UCmem_journal.element[head].addr,
+        (unsigned) bx_debugger.UCmem_journal.element[head].value);
+      dbg_printf ( "Error: slave:  op=W len=%u addr=0x%x val=0x%x\n",
+        (unsigned) 1, (unsigned) addr, (unsigned) value);
+      return;
+    }
+    // slave UCmem op in sync with journaled master op, delete this entry
+    bx_debugger.UCmem_journal.head++;
+    bx_debugger.UCmem_journal.size--;
+  }
+}
+
+void bx_dbg_async_pin_request(unsigned what, bx_bool val)
+{
+  // Request from IO devices for change in pin external to CPU.
+  // This is pended until CPU ack's with bx_dbg_async_pin_ack().
+
+  if (bx_debugger.master_slave_mode != BX_DBG_MASTER_MODE) {
+    dbg_printf ( "Error: dbg_async_pin_request not in master mode.\n");
+    bx_dbg_exit(1);
+  }
+
+  switch (what) {
+    case BX_DBG_ASYNC_PENDING_A20:
+      // Q pending status
+      bx_guard.async_changes_pending.which |= BX_DBG_ASYNC_PENDING_A20;
+      bx_guard.async_changes_pending.a20    = val;
+      return;
+
+    case BX_DBG_ASYNC_PENDING_RESET:
+    case BX_DBG_ASYNC_PENDING_NMI:
+    default:
+      dbg_printf ( "Error: set_async_pin: unhandled case.\n");
+      bx_dbg_exit(1);
+  }
+}
+
+
+void bx_dbg_async_pin_ack(unsigned what, bx_bool val)
+{
+  // Acknowledgement from master simulator for pending change in pin
+  // external to CPU.
+
+  if (bx_debugger.master_slave_mode != BX_DBG_MASTER_MODE) {
+    dbg_printf ( "Error: dbg_async_pin_ack: not master mode.\n");
+    bx_dbg_exit(1);
+  }
+
+  switch (what) {
+    case BX_DBG_ASYNC_PENDING_A20:
+      // get rid of pending status
+      bx_guard.async_changes_pending.which &= ~BX_DBG_ASYNC_PENDING_A20;
+      // notify pc_system of change
+      bx_pc_system.set_enable_a20(val);
+      if (BX_CPU(bx_debugger.master)->set_A20)
+        BX_CPU(bx_debugger.master)->set_A20(val);
+      bx_dbg_journal_a20_event(val);
+      return;
+
+    case BX_DBG_ASYNC_PENDING_RESET:
+    case BX_DBG_ASYNC_PENDING_NMI:
+    default:
+      dbg_printf ( "Error: set_async_pin: unhandled case.\n");
+      bx_dbg_exit(1);
+  }
+}
+
+Bit32u bx_dbg_inp(Bit16u addr, unsigned len)
+{
+  Bit32u value;
+  unsigned tail, head;
+
+  if ( bx_debugger.master_slave_mode == BX_DBG_MASTER_MODE ) {
+    if (!bx_debugger.fast_forward_mode) {
+      if (bx_debugger.IO_journal.size >= BX_DBG_IO_JOURNAL_SIZE) {
+        dbg_printf ( "dbg_inp: journal full.\n");
+        bx_dbg_exit(0);
+      }
+
+      if (bx_debugger.IO_journal.size == 0) {
+        // start off point head & tail at same element
+        bx_debugger.IO_journal.head = 0;
+        tail = bx_debugger.IO_journal.tail = 0;
+      }
+      else {
+        tail = bx_debugger.IO_journal.tail + 1;
+      }
+      if (tail >= BX_DBG_IO_JOURNAL_SIZE) {
+        dbg_printf ( "dbg_inp: journal wrapped.\n");
+        bx_dbg_exit(0);
+      }
+
+      value = bx_pc_system.inp(addr, len);
+      bx_debugger.IO_journal.element[tail].op    = BX_READ;
+      bx_debugger.IO_journal.element[tail].len   = (Bit8u) len;
+      bx_debugger.IO_journal.element[tail].addr  = addr;
+      bx_debugger.IO_journal.element[tail].value = value;
+      if (bx_debugger.IO_journal.size)
+        bx_debugger.IO_journal.tail++;
+      bx_debugger.IO_journal.size++;
+//dbg_printf ( "MASTER IN: head:%u tail%u size:%u\n",
+//  bx_debugger.IO_journal.head,
+//  bx_debugger.IO_journal.tail,
+//  bx_debugger.IO_journal.size);
+      return(value);
+    } else {
+      value = bx_pc_system.inp(addr, len);
+      return(value);
+    }
+  }
+  else {
+    if (bx_debugger.IO_journal.size == 0) {
+      dbg_printf ( "Error: dbg_inp: journal empty.\n");
+      return(0xffffffff);
+    }
+    head = bx_debugger.IO_journal.head;
+    value = bx_debugger.IO_journal.element[head].value;
+
+    if ((bx_debugger.IO_journal.element[head].op != BX_READ) ||
+        (bx_debugger.IO_journal.element[head].len != len) ||
+        (bx_debugger.IO_journal.element[head].addr != addr) ) {
+      dbg_printf ( "Error: dbg_inp: out of sync with journal.\n");
+      dbg_printf ( "Error: master: op=%3s len=%u addr=0x%x\n",
+        (bx_debugger.IO_journal.element[head].op==BX_WRITE) ? "OUT" : "IN",
+        (unsigned) bx_debugger.IO_journal.element[head].len,
+        (unsigned) bx_debugger.IO_journal.element[head].addr);
+      dbg_printf ( "Error: slave:  op=OUT len=%u addr=0x%x\n",
+        (unsigned) len, (unsigned) addr);
+      return(0xffffffff);
+    }
+    // slave IO op in sync with journaled master op, delete this entry
+    bx_debugger.IO_journal.head++;
+    bx_debugger.IO_journal.size--;
+// dbg_printf ( "SLAVE   IN: head:%u tail%u size:%u\n",
+//   bx_debugger.IO_journal.head,
+//   bx_debugger.IO_journal.tail,
+//   bx_debugger.IO_journal.size);
+    return(value);
+  }
+}
+
+void bx_dbg_outp(Bit16u addr, Bit32u value, unsigned len)
+{
+  unsigned tail, head;
+
+  if ( bx_debugger.master_slave_mode == BX_DBG_MASTER_MODE ) {
+    if (!bx_debugger.fast_forward_mode) {
+      if (bx_debugger.IO_journal.size >= BX_DBG_IO_JOURNAL_SIZE) {
+        dbg_printf ( "dbg_outp: IO journal full.\n");
+        bx_dbg_exit(0);
+      }
+
+      if (bx_debugger.IO_journal.size == 0) {
+        // start off point head & tail at same element
+        bx_debugger.IO_journal.head = 0;
+        tail = bx_debugger.IO_journal.tail = 0;
+      }
+      else {
+        tail = bx_debugger.IO_journal.tail + 1;
+      }
+      if (tail >= BX_DBG_IO_JOURNAL_SIZE) {
+        dbg_printf ( "dbg_outp: IO journal wrapped.\n");
+        bx_dbg_exit(0);
+      }
+
+      bx_debugger.IO_journal.element[tail].op    = BX_WRITE;
+      bx_debugger.IO_journal.element[tail].len   = (Bit8u) len;
+      bx_debugger.IO_journal.element[tail].addr  = addr;
+      bx_debugger.IO_journal.element[tail].value = value;
+      if (bx_debugger.IO_journal.size)
+        bx_debugger.IO_journal.tail++;
+      bx_debugger.IO_journal.size++;
+      bx_pc_system.outp(addr, value, len);
+      if (doit)
+        dbg_printf ( "master: IO journal size now %u\n", bx_debugger.IO_journal.size);
+    } else {
+      bx_pc_system.outp(addr, value, len);
+    }
+  }
+  else {
+    if (bx_debugger.IO_journal.size == 0) {
+      dbg_printf ( "Error: dbg_outp: journal empty.\n");
+      return;
+    }
+    head = bx_debugger.IO_journal.head;
+
+    if ((bx_debugger.IO_journal.element[head].op != BX_WRITE) ||
+        (bx_debugger.IO_journal.element[head].len != len) ||
+        (bx_debugger.IO_journal.element[head].addr != addr) ||
+        (bx_debugger.IO_journal.element[head].value != value) ) {
+      dbg_printf ( "Error: dbg_outp: out of sync with journal.\n");
+      dbg_printf ( "Error: master: op=%3s len=%u addr=0x%x val=0x%x\n",
+        (bx_debugger.IO_journal.element[head].op==BX_WRITE) ? "OUT" : "IN",
+        (unsigned) bx_debugger.IO_journal.element[head].len,
+        (unsigned) bx_debugger.IO_journal.element[head].addr,
+        (unsigned) bx_debugger.IO_journal.element[head].value);
+      dbg_printf ( "Error: slave:  op=OUT len=%u addr=0x%x val=0x%x\n",
+        (unsigned) len, (unsigned) addr, (unsigned) value);
+      return;
+    }
+    // slave IO op in sync with journaled master op, delete this entry
+    bx_debugger.IO_journal.head++;
+    bx_debugger.IO_journal.size--;
+    if (doit)
+      dbg_printf ( "slave: IO journal size now %u\n", bx_debugger.IO_journal.size);
+  }
+}
+
+void bx_dbg_raise_HLDA(void)
+{
+  dbg_printf ( "dbg_HLDA called\n");
+  bx_dbg_exit(0);
+}
+
+Bit8u bx_dbg_IAC(void)
+{
+  // Convience routine.  bochs skips this, and calls the PIC code
+  // directly.  This is for other simulators to interface to the
+  // the PIC code.
+  unsigned iac;
+
+  iac = BX_PIC_AIC ();
+  return(iac);
+}
+
+void bx_dbg_set_INTR(bx_bool b)
+{
+  if ( bx_debugger.master_slave_mode == BX_DBG_SLAVE_MODE ) {
+    dbg_printf ( "Error: set_INTR in slave mode.\n");
+    bx_dbg_exit(1);
+  }
+
+  bx_pc_system.INTR = b;
+  BX_CPU(bx_debugger.master)->set_INTR(b);
+}
+
+#endif
+
+void bx_dbg_diff_memory(void)
+{
+#if BX_NUM_SIMULATORS < 2
+  printf("diff-memory supported only in cosimulation mode\n");
+#else
+  int num_pages = bx_options.memory.Osize->get () * 1024 / 4;
+  for (int i = 0; i < num_pages; i++) {
+    BX_CPU(dbg_cpu)->dbg_dirty_pages[i] = 1;
+  }
+  if (bx_dbg_compare_sim_memory())
+    printf("[diff-memory] Diff detected\n");
+  else
+    printf("[diff-memory] No diff detected\n");
+#endif /* NUM_SIMULATORS < 2 */
+}
+
+void bx_dbg_sync_memory(bx_bool set)
+{
+#if BX_NUM_SIMULATORS < 2
+  printf("sync-memory supported only in cosimulation mode\n");
+#else
+  bx_debugger.compare_at_sync.memory = set;
+  printf("Memory sync %s\n", (set) ? "enabled" : "disabled");
+#endif
+}
+
+void bx_dbg_sync_cpu(bx_bool set)
+{
+#if BX_NUM_SIMULATORS < 2
+  printf("sync-cpu supported only in cosimulation mode\n");
+#else
+  bx_debugger.compare_at_sync.cpu = set;
+  printf("Register file sync %s\n", (set) ? "enabled" : "disabled");
+#endif
+}
+
+void bx_dbg_fast_forward(Bit32u num)
+{
+#if BX_NUM_SIMULATORS < 2
+  printf("fast-forward supported only in cosimulation mode\n");
+#else
+  printf("Entering fast-forward mode\n");
+
+  // Bit32u save_icount_quantum = bx_debugger.icount_quantum;
+  // bx_debugger.icount_quantum = num;
+
+  bx_guard.interrupt_requested = 0;
+
+  bx_debugger.fast_forward_mode = 1;
+  for (Bit32u e = 0; e < num; e += bx_debugger.icount_quantum)
+    if (!bx_dbg_cosimulateN(bx_debugger.icount_quantum))
+      break;
+  bx_debugger.fast_forward_mode = 0;
+  // bx_debugger.icount_quantum = save_icount_quantum;
+
+  DEV_vga_refresh();
+
+  printf("Copying CPU...\n");
+  bx_dbg_cpu_t cpu;
+  if (!BX_CPU(0)->dbg_get_cpu(&cpu) || !BX_CPU(1)->dbg_set_cpu(&cpu))
+    printf("Error copying CPU data!\n");
+
+  printf("Copying memory...\n");
+  int num_pages = bx_options.memory.Osize->get () * 1024 / 4;
+  for (int i = 0; i < num_pages; i++) {
+    if (BX_CPU(0)->dbg_dirty_pages[i]) {
+      Bit32u page_start = i * 1024 * 4;
+      printf("Copying page %08x\n", page_start);
+      extern Bit8u* SIM1_GET_PHYS_PTR(Bit32u page_start);
+      Bit8u* sim0_page_vec = bx_mem0.vector + page_start;
+      Bit8u* sim1_page_vec = SIM1_GET_PHYS_PTR(page_start);
+      memcpy(sim1_page_vec, sim0_page_vec, 1024 * 4);
+    }
+  }
+
+  printf("Taking async events...\n");
+
+  printf("Exiting fast-forward mode\n");
+#endif
+}
+
+extern Bit32u conv_4xBit8u_to_Bit32u(const Bit8u* buf);
+
+/*
+  (mch) Print various info for logical address.
+*/
+void bx_dbg_info_address(Bit32u seg_reg_num, Bit32u offset)
+{
+#if BX_NUM_SIMULATORS < 2
+  printf("addr-info only supported in cosim configuration.\n");
+#else
+  for (int sim = 0; sim < 2; sim++) 
+  {
+    /* Find page table base address */
+    bx_dbg_cpu_t regs;
+    BX_CPU(sim)->dbg_get_cpu(&regs);
+    Bit32u base = regs.cr3 & ~0xfff;
+
+    Bit8u buf[4];
+    Bit32u directory_addr = base + (offset >> 22) * 4;
+    Bit32u directory;
+    if (BX_CPU(sim)->mem->dbg_fetch_mem(directory_addr, 4, buf)) {
+      directory = conv_4xBit8u_to_Bit32u(buf);
+      Bit32u table_addr = (directory & ~0xfff) + ((offset >> 12) & 0x3ff) * 4;
+      Bit32u table;
+
+      printf("[%s] ", SIM_NAME(sim));
+      printf("PDE: %08x (", directory);
+      printf("%s,  %s, %s, %s, %s)",
+             (directory & 1) ? "Present" : "Not present",
+             (directory & 2) ? "Read/Write" : "Read-only",
+             (directory & 4) ? "User" : "Supervisor",
+             (directory & (1 << 5)) ? "Accessed" : "-",
+             (directory & (1 << 6)) ? "Dirty" : "-");
+
+      if (directory & 1) {
+        if (BX_CPU(sim)->mem->dbg_fetch_mem(table_addr, 4, buf)) {
+          table = conv_4xBit8u_to_Bit32u(buf);
+
+          printf(", PTE: %08x (", table);
+          printf("%s,  %s, %s, %s, %s)\n",
+                 (table & 1) ? "Present" : "Not present",
+                 (table & 2) ? "Read/Write" : "Read-only",
+                 (table & 4) ? "User" : "Supervisor",
+                 (table & (1 << 5)) ? "Accessed" : "-",
+                 (table & (1 << 6)) ? "Dirty" : "-");
+        } else {
+          printf("[%s] Could not read from physical address %08x\n",
+                 SIM_NAME(sim), directory_addr);
+          return;
+        }
+      } else {
+        printf("\n");
+      }
+    } else {
+      printf("[%s] Could not read from physical address %08x\n",
+             SIM_NAME(sim), directory_addr);
+      return;
+    }
+  }
+#endif
+}
diff -uBbwNpr bochs-nocosim/bx_debug/dbg_main.cc bochs/bx_debug/dbg_main.cc
--- bochs-nocosim/bx_debug/dbg_main.cc	2006-01-25 22:57:42.921875000 +0200
+++ bochs/bx_debug/dbg_main.cc	2006-01-25 23:39:08.937500000 +0200
@@ -45,8 +45,18 @@ extern "C" {
 }
 #endif
 
+
+static unsigned doit = 0;
+
+#define SIM_NAME0 "bochs"
+#ifndef SIM_NAME1_STR
+#define SIM_NAME1_STR "sim1"
+#endif
+#define SIM_NAME(x) ((x == 0) ? SIM_NAME0 : SIM_NAME1_STR)
+
 // default CPU in the debugger.  For commands like "dump_cpu" it will
 // use the default instead of always dumping all cpus.
+
 Bit32u dbg_cpu = 0;
 
 bx_param_bool_c *sim_running;
@@ -58,9 +68,87 @@ static char tmp_buf_prev[512];
 static char *tmp_buf_ptr;
 static char *argv0 = NULL;
 
+#if BX_NUM_SIMULATORS >= 2
+#define BX_DBG_IO_JOURNAL_SIZE        1024
+#define BX_DBG_UCMEM_JOURNAL_SIZE     1024
+#define BX_DBG_ASYNC_JOURNAL_SIZE     1024
+#define BX_DBG_MASTER_MODE              10
+#define BX_DBG_SLAVE_MODE               11
+// #define BX_DBG_DEFAULT_ICOUNT_QUANTUM   50
+#define BX_DBG_DEFAULT_ICOUNT_QUANTUM   3 /* mch */
+
+static unsigned bx_dbg_cosimulateN(bx_dbg_icount_t count);
+static int      bx_dbg_compare_sim_iaddr(void);
+static bx_bool  bx_dbg_compare_sim_cpu(void);
+static bx_bool  bx_dbg_compare_sim_memory(void);
+static void     bx_dbg_journal_a20_event(unsigned val);
+#endif
+
 static FILE *debugger_log = NULL;
 
 static struct {
+#if BX_NUM_SIMULATORS >= 2
+  // some fields used only for cosimulation
+  unsigned icount_quantum;
+  unsigned master_slave_mode;
+  unsigned master, slave;
+  struct {
+    struct {
+      Bit8u    op;
+      Bit8u    len;
+      Bit16u   addr;
+      Bit32u   value;
+    } element[BX_DBG_IO_JOURNAL_SIZE];
+    unsigned size;
+    unsigned head, tail;
+  } IO_journal;
+
+  struct {
+    struct {
+      Bit8u    op;
+      Bit8u    len;
+      Bit32u   addr;
+      Bit32u   value;
+    } element[BX_DBG_UCMEM_JOURNAL_SIZE];
+    unsigned size;
+    unsigned head, tail;
+  } UCmem_journal;
+
+// need to handle DMA stuff in here...
+
+#define BX_DBG_ASYNC_JOURNAL_NONE   0
+#define BX_DBG_ASYNC_JOURNAL_A20    1
+#define BX_DBG_ASYNC_JOURNAL_IAC    2
+#define BX_DBG_ASYNC_JOURNAL_NMI    3
+#define BX_DBG_ASYNC_JOURNAL_RESET  4
+
+  // Asynchronous events at the boundaries they are *taken* by the master simulator.
+  // These are replayed back to the slave at the same boundaries.
+  struct {
+    struct {
+      unsigned        what; // A20, INTR, NMI, RESET, IAC, ...
+      bx_dbg_icount_t icount;
+      union {
+        struct {
+          unsigned val;
+        } a20, nmi, reset, iac;
+        // perhaps other more complex types here
+      } u;
+    } element[BX_DBG_ASYNC_JOURNAL_SIZE];
+    unsigned size;
+    unsigned head, tail;
+  } async_journal;
+
+  struct {
+    bx_bool iaddr;
+    bx_bool cpu;
+    bx_bool memory;
+  } compare_at_sync;
+
+  bx_bool fast_forward_mode;
+
+#endif  // #if BX_NUM_SIMULATORS >= 2
+
   // some fields used for single CPU debugger
   bx_bool  auto_disassemble;
   unsigned disassemble_size;
@@ -77,7 +165,19 @@ static struct {
 #endif
 } bx_debugger;
 
-#define BX_DBG_DEFAULT_ICOUNT_QUANTUM   3 /* mch */
+
+
+// cosim commands for handling of comparison of simulator
+// environments when both simulators have reached a common
+// point (synchronized).
+
+// cosim compare_at_sync iaddr  (default is on)
+// cosim compare_at_sync cpu    (default is off)
+// cosim compare_at_sync memory (default is off)
+// cosim compare iaddr
+// cosim compare cpu
+// cosim compare memory
+
 
 typedef struct {
   FILE    *fp;
@@ -97,8 +197,10 @@ static void bx_get_command(void);
 static void bx_dbg_print_guard_results();
 static void bx_dbg_breakpoint_changed(void);
 
+bx_dbg_callback_t bx_dbg_callback[BX_NUM_SIMULATORS];
 bx_guard_t        bx_guard;
 
+
 // DMA stuff
 void bx_dbg_post_dma_reports(void);
 #define BX_BATCH_DMA_BUFSIZE 512
@@ -138,8 +240,10 @@ void dbg_printf (const char *fmt, ...)
 
 int bx_dbg_main(int argc, char *argv[])
 {
-  int i, bochs_argc=0;
+  int i, bochs_argc=0, sim1_argc=0, sim2_argc=0;
   char **bochs_argv = NULL;
+  char **sim1_argv = NULL;
+  char **sim2_argv = NULL;
   argc = 1;
   
   setbuf (stdout, NULL);
@@ -148,11 +252,29 @@ int bx_dbg_main(int argc, char *argv[])
   bx_dbg_batch_dma.this_many = 1;
   bx_dbg_batch_dma.Qsize     = 0;
 
+  // initialize callback functions, and guard environment
+  memset(bx_dbg_callback, 0, sizeof(bx_dbg_callback));
   memset(&bx_guard, 0, sizeof(bx_guard));
   bx_guard.async.irq = 1;
   bx_guard.async.dma = 1;
 
   memset(&bx_debugger, 0, sizeof(bx_debugger));
+#if BX_NUM_SIMULATORS >= 2
+  bx_debugger.icount_quantum = BX_DBG_DEFAULT_ICOUNT_QUANTUM;
+  bx_debugger.IO_journal.size = 0;
+  bx_debugger.IO_journal.head = 0;
+  bx_debugger.IO_journal.tail = 0;
+  bx_debugger.UCmem_journal.size = 0;
+  bx_debugger.UCmem_journal.head = 0;
+  bx_debugger.UCmem_journal.tail = 0;
+  bx_debugger.async_journal.size = 0;
+  bx_debugger.async_journal.head = 0;
+  bx_debugger.async_journal.tail = 0;
+  bx_debugger.master = 0;
+  bx_debugger.slave  = 1;
+  bx_debugger.compare_at_sync.iaddr  = 1;
+  bx_debugger.fast_forward_mode = 0;
+#endif
   bx_debugger.auto_disassemble = 1;
   bx_debugger.disassemble_size = 0;
   bx_debugger.default_display_format = 'x';
@@ -166,7 +289,11 @@ int bx_dbg_main(int argc, char *argv[])
   bx_debug_rc_fname[0] = '\0';
 
   bochs_argv = (char **) &argv[0];
+  sim1_argv = bochs_argv;  // start out with something reasonable
+  sim2_argv = bochs_argv;  // start out with something reasonable
   bochs_argc = 1;
+  sim1_argc = 1;
+  sim2_argc = 1;
 
   // process "-rc pathname" option, if it exists
   i = 1;
@@ -182,6 +309,41 @@ int bx_dbg_main(int argc, char *argv[])
     bochs_argv = (char **) &argv[2];
   }
 
+  // process options to bochs framework
+  for (; i<argc; i++) {
+    if (strcmp(argv[i], "-sim1") == 0) {
+      break;
+    }
+    else if (strcmp(argv[i], "-sim2") == 0) {
+      break;
+    }
+    bochs_argc++;
+  }
+
+  if (i<argc) {  // more args to process
+    // process options to each CPU simulator
+    if (strcmp(argv[i], "-sim1") == 0) {
+process_sim1:
+      sim1_argv = (char **) &argv[i];
+      i++;
+      for (; i<argc; i++) {
+        if (strcmp(argv[i], "-sim2") == 0)
+          goto process_sim2;
+        sim1_argc++;
+      }
+    }
+    else if (strcmp(argv[i], "-sim2") == 0) {
+process_sim2:
+      sim2_argv = (char **) &argv[i];
+      i++;
+      for (; i<argc; i++) {
+        if (strcmp(argv[i], "-sim1") == 0)
+          goto process_sim1;
+        sim2_argc++;
+      }
+    }
+  }
+
   bx_infile_stack_index = 0;
   bx_infile_stack[0].fp = stdin;
   strncpy(bx_infile_stack[0].fname, argv[0], BX_MAX_PATH);
@@ -215,13 +377,36 @@ int bx_dbg_main(int argc, char *argv[])
   memset(bx_disasm_ibuf, 0, sizeof(bx_disasm_ibuf));
 #endif
 
+  BX_SIM1_INIT(&bx_dbg_callback[0], sim1_argc, sim1_argv);
+#if BX_NUM_SIMULATORS >= 2
+  BX_SIM2_INIT(&bx_dbg_callback[1], sim2_argc, sim2_argv);
+#endif
+
   // parse any remaining args in the usual way
   bx_parse_cmdline (1, bochs_argc, bochs_argv);
 
   // initialize hardware
   bx_init_hardware();
 
-  // Moved from main.cc
+#if BX_NUM_SIMULATORS >= 2
+  bx_debugger.compare_at_sync.cpu    = 0;
+  bx_debugger.compare_at_sync.memory = 0;
+#endif
+
+  // call init routines for each CPU+mem simulator
+  // initialize for SMP. one memory, multiple processors.
+
+#if BX_NUM_SIMULATORS > 1
+#error cosimulation not supported until SMP stuff settles
+  BX_MEM(1) = new BX_MEM_C ();
+  BX_CPU(1) = new BX_CPU_C (BX_MEM(1));
+  BX_CPU(1)->reset(BX_RESET_HARDWARE);
+  BX_MEM(1)->init_memory(bx_options.memory.Osize->get () * 1024*1024);
+  BX_MEM(1)->load_ROM(bx_options.rom.path->getptr (), bx_options.rom.address->get (), 1);
+  BX_MEM(1)->load_ROM(bx_options.vgarom.path->getptr (), 0xc0000, 2);
+#endif
+
+  // (mch) Moved from main.cc
   DEV_init_devices();
   DEV_reset_devices(BX_RESET_HARDWARE);
   bx_gui->init_signal_handlers ();
@@ -524,11 +709,16 @@ void  bx_debug_break ()
 
 void bx_dbg_exit(int code)
 {
-  BX_DEBUG(("dbg: before exit" ));
+  BX_DEBUG(("dbg: before sim1_exit" ));
   for (int cpu=0; cpu < BX_SMP_PROCESSORS; cpu++) {
     if (BX_CPU(cpu)) BX_CPU(cpu)->atexit();
   }
 
+#if BX_NUM_SIMULATORS >= 2
+  dbg_printf("before sim2_exit\n");
+  if (BX_CPU(1)) BX_CPU(1)->atexit();
+#endif
+
   bx_atexit();
   BX_EXIT(code);
 }
@@ -570,6 +761,17 @@ void bx_dbg_trace_reg_off_command(void)
 void bx_dbg_ptime_command(void)
 {
   dbg_printf("ptime: " FMT_LL "d\n", bx_pc_system.time_ticks());
+#if BX_NUM_SIMULATORS >= 2
+  dbg_printf (
+#if BX_DBG_ICOUNT_SIZE == 32
+    "Last synchronized icount was %lu\n",
+    (unsigned long) bx_debugger.last_sync_icount
+#else  // BX_DBG_ICOUNT_SIZE == 64
+    "Last synchronized icount was %Lu\n",
+    (unsigned long long) bx_debugger.last_sync_icount
+#endif /* BX_DBG_ICOUNT_SIZE == 32 */
+  );
+#endif /* BX_NUM_SIMULATORS >= 2 */
 }
 
 int timebp_timer = -1;
@@ -1041,6 +1243,14 @@ void bx_dbg_continue_command(void)
 
 one_more:
 
+#if BX_NUM_SIMULATORS >= 2
+  bx_guard.interrupt_requested = 0;
+  bx_guard.special_unwind_stack = 0;
+  while (1) {
+    if ( !bx_dbg_cosimulateN(bx_debugger.icount_quantum) )
+      break;
+    }
+#else
   bx_guard.icount = 0;
   // I must guard for ICOUNT or one CPU could run forever without giving
   // the others a chance.
@@ -1115,6 +1325,7 @@ one_more:
     BX_TICKN(max_executed);
 #endif /* BX_SUPPORT_SMP */
   }
+#endif /* BX_NUM_SIMULATORS */
 
   sim_running->set (0);
   SIM->refresh_ci ();
@@ -1141,6 +1352,11 @@ void bx_dbg_stepN_command(bx_dbg_icount_
   // is printed, we will return to config mode.
   SIM->set_display_mode (DISP_MODE_SIM);
 
+#if BX_NUM_SIMULATORS >= 2
+  bx_guard.interrupt_requested = 0;
+  bx_guard.special_unwind_stack = 0;
+  bx_dbg_cosimulateN(count);
+#else
   // single CPU
   bx_guard.guard_for |= BX_DBG_GUARD_ICOUNT; // looking for icount
   bx_guard.guard_for |= BX_DBG_GUARD_CTRL_C; // or Ctrl-C
@@ -1159,6 +1375,7 @@ void bx_dbg_stepN_command(bx_dbg_icount_
     BX_TICK1 ();
 #endif
   }
+#endif
 
   BX_INSTR_DEBUG_PROMPT();
   bx_dbg_print_guard_results();
@@ -1822,7 +2039,7 @@ void dbg_printf_binary (char *format, Bi
 }
 
 void bx_dbg_examine_command(char *command, char *format, bx_bool format_passed,
-               Bit32u addr, bx_bool addr_passed)
+               Bit32u addr, bx_bool addr_passed, int simulator)
 {
   unsigned repeat_count, i;
   char ch, display_format, unit_size;
@@ -1837,7 +2054,10 @@ void bx_dbg_examine_command(char *comman
   bx_bool is_linear;
   unsigned char databuf[8];
 
-  printf("[bochs]:\n");
+  if (simulator == 0)
+    printf("[%s]:\n", SIM_NAME0);
+  else
+    printf("[%s]:\n", SIM_NAME1_STR);
 
   // If command was the extended "xp" command, meaning eXamine Physical memory,
   // then flag memory address as physical, rather than linear.
@@ -1934,6 +2154,10 @@ void bx_dbg_examine_command(char *comman
     bx_debugger.default_unit_size      = unit_size;
   }
 
+  //dbg_printf("  repeat count was %u\n", repeat_count);
+  //dbg_printf("  display_format = '%c'\n", display_format);
+  //dbg_printf("  unit_size      = '%c'\n", unit_size);
+
   if ( (display_format == 'i') || (display_format == 's') ) {
     dbg_printf("error: dbg_examine: 'i' and 's' formats not supported.\n");
     return;
@@ -1996,7 +2220,7 @@ void bx_dbg_examine_command(char *comman
       dbg_printf(" ");
 
     if (is_linear) {
-      BX_CPU(0)->dbg_xlate_linear2phy(addr, &paddr, &paddr_valid);
+      BX_CPU(simulator)->dbg_xlate_linear2phy(addr, &paddr, &paddr_valid);
       if (!paddr_valid) {
         dbg_printf("error: examine memory: no tranlation for linear-to-phy mem available.\n");
         return;
@@ -2006,7 +2230,7 @@ void bx_dbg_examine_command(char *comman
       paddr = addr;  // address is already physical address
     }
 
-    BX_MEM(0)->dbg_fetch_mem(paddr, data_size, databuf);
+    BX_MEM(simulator)->dbg_fetch_mem(paddr, data_size, databuf);
     //FIXME HanishKVC The char display for data to be properly integrated
     //      so that repeat_count, columns, etc. can be set or used properly.
     //      Also for data_size of 2 and 4 how to display the individual
@@ -2564,6 +2788,42 @@ void bx_dbg_instrument_command(const cha
 #endif
 }
 
+void bx_dbg_loader_command(char *path_quoted)
+{
+  size_t len;
+
+  // skip beginning double quote
+  if (path_quoted[0] == '"')
+    path_quoted++;
+
+  // null out ending quote
+  len = strlen(path_quoted);
+  if (path_quoted[len - 1] == '"')
+    path_quoted[len - 1] = '\0';
+
+#if BX_USE_LOADER
+  {
+    bx_loader_misc_t loader_misc;
+    bx_dbg_callback[0].loader(path_quoted, &loader_misc);
+#if 0
+    dbg_printf("dr0: 0x%08x\n", loader_misc.dr0);
+    dbg_printf("dr1: 0x%08x\n", loader_misc.dr1);
+    dbg_printf("dr2: 0x%08x\n", loader_misc.dr2);
+    dbg_printf("dr3: 0x%08x\n", loader_misc.dr3);
+    dbg_printf("dr6: 0x%08x\n", loader_misc.dr6);
+    dbg_printf("dr7: 0x%08x\n", loader_misc.dr7);
+#endif
+    bx_cpu.dr0 = loader_misc.dr0;
+    bx_cpu.dr1 = loader_misc.dr1;
+    bx_cpu.dr2 = loader_misc.dr2;
+    bx_cpu.dr3 = loader_misc.dr3;
+    bx_cpu.dr7 = loader_misc.dr7;
+  }
+#else
+  dbg_printf("Error: loader not implemented.\n");
+#endif
+}
+
 void bx_dbg_doit_command(unsigned n)
 {
   // generic command to add temporary hacks to
@@ -2584,10 +2844,24 @@ void bx_dbg_crc_command(Bit32u addr1, Bi
   }
 
   if (!BX_MEM(0)->dbg_crc32(crc32, addr1, addr2, &crc1)) {
-    dbg_printf("could not CRC memory\n");
+    dbg_printf("sim0: could not CRC memory\n");
     return;
   }
+#if BX_NUM_SIMULATORS == 1
   dbg_printf("0x%lx\n", crc1);
+#else
+  if (!BX_MEM(1)->dbg_crc32(crc32, addr1, addr2, &crc2)) {
+    dbg_printf("sim1: could not CRC memory\n");
+    return;
+  }
+  if (crc1 == crc2) {
+    dbg_printf("CRC same: 0x%x\n", (unsigned) crc1);
+  }
+  else {
+    dbg_printf("CRC different: sim0=0x%x, sim1=0x%x\n",
+            (unsigned) crc1, (unsigned) crc2);
+  }
+#endif
 }
 
 void bx_dbg_info_dirty_command(void)
@@ -2931,10 +3205,51 @@ void bx_dbg_info_vga()
 
 void bx_dbg_iac_report(unsigned vector, unsigned irq)
 {
+#if BX_NUM_SIMULATORS > 1
+  unsigned tail, master;
+#endif
+
+if (doit) dbg_printf("iac report: vector=%u\n", vector);
+
   if (bx_guard.report.irq) {
     dbg_printf("event icount=%u IRQ irq=%u vec=%x\n",
       (unsigned) BX_CPU(dbg_cpu)->guard_found.icount, irq, vector);
   }
+
+#if BX_NUM_SIMULATORS > 1
+  if (bx_debugger.master_slave_mode == BX_DBG_SLAVE_MODE ) {
+    dbg_printf("Error: iac_report: in slave mode.\n");
+    bx_dbg_exit(1);
+  }
+
+  // Master simulator mode
+  if (bx_debugger.async_journal.size >= BX_DBG_ASYNC_JOURNAL_SIZE) {
+    dbg_printf("Error: iac: async journal full.\n");
+    bx_dbg_exit(1);
+  }
+
+  if (bx_debugger.async_journal.size == 0) {
+    // start off point head & tail at same element
+    bx_debugger.async_journal.head = 0;
+    tail = bx_debugger.async_journal.tail = 0;
+  }
+  else {
+    tail = bx_debugger.async_journal.tail + 1;
+  }
+  if (tail >= BX_DBG_ASYNC_JOURNAL_SIZE) {
+    dbg_printf("Error: iac_report: journal wrapped.\n");
+    bx_dbg_exit(0);
+  }
+
+  master = bx_debugger.master;
+  bx_debugger.async_journal.element[tail].what = BX_DBG_ASYNC_JOURNAL_IAC;
+  bx_debugger.async_journal.element[tail].icount = bx_guard_found[master].icount;
+  bx_debugger.async_journal.element[tail].u.iac.val = vector;
+
+  if (bx_debugger.async_journal.size)
+    bx_debugger.async_journal.tail++;
+  bx_debugger.async_journal.size++;
+#endif
 }
 
 void bx_dbg_a20_report(unsigned val)
@@ -2955,6 +3270,8 @@ void bx_dbg_io_report(Bit32u addr, unsig
       (op==BX_READ) ? "read" : "write",
       (unsigned) val);
   }
+
+  // nothing else to do.  bx_dbg_inp() and bx_dbg_outp() do the journaling.
 }
 
 void bx_dbg_ucmem_report(Bit32u addr, unsigned size, unsigned op, Bit32u val)
@@ -2967,6 +3284,8 @@ void bx_dbg_ucmem_report(Bit32u addr, un
       (op==BX_READ) ? "read" : "write",
       (unsigned) val);
   }
+  // nothing else to do.  bx_dbg_ucmem_read() and bx_dbg_ucmem_write()
+  // do the journaling.
 }
 
 void bx_dbg_dma_report(Bit32u addr, unsigned len, unsigned what, Bit32u val)
diff -uBbwNpr bochs-nocosim/bx_debug/debug.h bochs/bx_debug/debug.h
--- bochs-nocosim/bx_debug/debug.h	2006-01-25 22:58:39.187500000 +0200
+++ bochs/bx_debug/debug.h	2006-01-25 23:35:58.671875000 +0200
@@ -29,6 +29,11 @@
 #include "config.h"
 #include "osdep.h"
 
+#if BX_USE_LOADER
+#include "loader_misc.h"
+void bx_dbg_loader(char *path, bx_loader_misc_t *misc_ptr);
+#endif
+
 #if BX_DBG_ICOUNT_SIZE == 32
   typedef Bit32u bx_dbg_icount_t;
 #elif BX_DBG_ICOUNT_SIZE == 64
@@ -143,6 +148,12 @@ void bx_dbg_trace_reg_on_command(void);
 void bx_dbg_trace_reg_off_command(void);
 void bx_dbg_ptime_command(void);
 void bx_dbg_timebp_command(bx_bool absolute, Bit64u time);
+void bx_dbg_diff_memory(void);
+void bx_dbg_always_check(Bit32u page_start, bx_bool on);
+void bx_dbg_sync_memory(bx_bool set);
+void bx_dbg_sync_cpu(bx_bool set);
+void bx_dbg_fast_forward(Bit32u num);
+void bx_dbg_info_address(Bit32u seg_reg_num, Bit32u offset);
 #define MAX_CONCURRENT_BPS 5
 extern int timebp_timer;
 extern Bit64u timebp_queue[MAX_CONCURRENT_BPS];
@@ -189,7 +200,7 @@ void bx_dbg_info_flags(void);
 void bx_dbg_info_linux_command(void);
 void bx_dbg_info_symbols_command(char *Symbol);
 void bx_dbg_examine_command(char *command, char *format, bx_bool format_passed,
-                    Bit32u addr, bx_bool addr_passed);
+                    Bit32u addr, bx_bool addr_passed, int simulator);
 void bx_dbg_setpmem_command(Bit32u addr, unsigned len, Bit32u val);
 void bx_dbg_set_symbol_command(char *symbol, Bit32u val);
 void bx_dbg_query_command(char *);
@@ -198,10 +209,11 @@ void bx_dbg_dump_cpu_command(void);
 void bx_dbg_set_cpu_command(void);
 void bx_dbg_disassemble_command(const char *,bx_num_range);
 void bx_dbg_instrument_command(const char *);
+void bx_dbg_loader_command(char *);
 void bx_dbg_doit_command(unsigned);
 void bx_dbg_crc_command(Bit32u addr1, Bit32u addr2);
 extern bx_bool watchpoint_continue;
-void bx_dbg_linux_syscall (unsigned which_cpu);
+void bx_dbg_linux_syscall (void);
 void bx_dbg_info_ne2k(int page, int reg);
 void bx_dbg_info_pic(void);
 void bx_dbg_info_vga(void);
@@ -423,12 +437,71 @@ typedef struct {
     unsigned inhibit_mask;
 } bx_dbg_cpu_t;
 
+
+typedef struct {
+  // call back functions specific to each simulator
+  bx_bool (*setphymem)(Bit32u addr, unsigned len, Bit8u *buf);
+  bx_bool (*getphymem)(Bit32u addr, unsigned len, Bit8u *buf);
+  void    (*xlate_linear2phy)(Bit32u linear, Bit32u *phy, bx_bool *valid);
+  bx_bool (*set_reg)(unsigned reg, Bit32u val);
+  Bit32u  (*get_reg)(unsigned reg);
+  bx_bool (*get_sreg)(bx_dbg_sreg_t *sreg, unsigned sreg_no);
+  bx_bool (*set_cpu)(bx_dbg_cpu_t *cpu);
+  bx_bool (*get_cpu)(bx_dbg_cpu_t *cpu);
+  unsigned       dirty_page_tbl_size;
+  unsigned char *dirty_page_tbl;
+  void    (*atexit)(void);
+  unsigned (*query_pending)(void);
+  void     (*execute)(void);
+  void     (*take_irq)(void);
+  void     (*take_dma)(void);
+  void     (*reset_cpu)(unsigned source);
+  void     (*init_mem)(int size_in_bytes);
+  void     (*load_ROM)(const char *path, Bit32u romaddress, Bit8u type);
+
+  // for asynchronous environment handling
+  void     (*set_A20)(unsigned val);
+  void     (*set_NMI)(unsigned val);
+  void     (*set_RESET)(unsigned val);
+  void     (*set_INTR)(unsigned val);
+  void     (*force_interrupt)(unsigned vector);
+
+#if BX_INSTRUMENTATION
+  void    (*instr_start)(void);
+  void    (*instr_stop)(void);
+  void    (*instr_reset)(void);
+  void    (*instr_print)(void);
+#endif
+#if BX_USE_LOADER
+  void    (*loader)(char *path, bx_loader_misc_t *misc_ptr);
+#endif
+  bx_bool (*crc32)(Bit32u (*f)(const Bit8u *buf, int len),
+                   Bit32u addr1, Bit32u addr2, Bit32u *crc);
+} bx_dbg_callback_t;
+
+extern bx_dbg_callback_t bx_dbg_callback[BX_NUM_SIMULATORS];
+
+void BX_SIM1_INIT(bx_dbg_callback_t *, int argc, char *argv[]);
+#ifdef BX_SIM2_INIT
+void BX_SIM2_INIT(bx_dbg_callback_t *, int argc, char *argv[]);
+#endif
+
+
 void bx_dbg_dma_report(Bit32u addr, unsigned len, unsigned what, Bit32u val);
 void bx_dbg_iac_report(unsigned vector, unsigned irq);
 void bx_dbg_a20_report(unsigned val);
 void bx_dbg_io_report(Bit32u addr, unsigned size, unsigned op, Bit32u val);
 void bx_dbg_ucmem_report(Bit32u addr, unsigned size, unsigned op, Bit32u val);
 
+Bit8u   bx_dbg_ucmem_read(Bit32u addr);
+void    bx_dbg_ucmem_write(Bit32u addr, Bit8u value);
+void    bx_dbg_async_pin_request(unsigned what, bx_bool val);
+void    bx_dbg_async_pin_ack(unsigned what, bx_bool val);
+Bit32u  bx_dbg_inp(Bit16u addr, unsigned len);
+void    bx_dbg_outp(Bit16u addr, Bit32u value, unsigned len);
+void    bx_dbg_raise_HLDA(void);
+Bit8u   bx_dbg_IAC(void);
+void    bx_dbg_set_INTR(bx_bool b);
 void bx_dbg_disassemble_current(int which_cpu, int print_time);
 
 int bx_dbg_symbolic_output(void); /* BW */
diff -uBbwNpr bochs-nocosim/bx_debug/lexer.l bochs/bx_debug/lexer.l
--- bochs-nocosim/bx_debug/lexer.l	2006-01-25 23:07:59.828125000 +0200
+++ bochs/bx_debug/lexer.l	2006-01-25 20:13:44.000000000 +0200
@@ -92,6 +92,7 @@ start           { bxlval.sval = strdup(b
 stop            { bxlval.sval = strdup(bxtext); return(BX_TOKEN_STOP); }
 reset           { bxlval.sval = strdup(bxtext); return(BX_TOKEN_RESET); }
 print           { bxlval.sval = strdup(bxtext); return(BX_TOKEN_PRINT); }
+loader          { bxlval.sval = strdup(bxtext); return(BX_TOKEN_LOADER); }
 doit            { bxlval.sval = strdup(bxtext); return(BX_TOKEN_DOIT); }
 trace-on        { bxlval.sval = strdup(bxtext); return(BX_TOKEN_TRACEON); }
 trace-off       { bxlval.sval = strdup(bxtext); return(BX_TOKEN_TRACEOFF); }
@@ -118,6 +119,12 @@ slist           { bxlval.sval = strdup(b
 global          { bxlval.sval = strdup(bxtext); return(BX_TOKEN_GLOBAL); }
 where           { bxlval.sval = strdup(bxtext); return(BX_TOKEN_WHERE); }
 print-string    { bxlval.sval = strdup(bxtext); return(BX_TOKEN_PRINT_STRING); }
+diff-memory     { bxlval.sval = strdup(bxtext); return(BX_TOKEN_DIFF_MEMORY); }
+sync-memory     { bxlval.sval = strdup(bxtext); return(BX_TOKEN_SYNC_MEMORY); }
+sync-cpu        { bxlval.sval = strdup(bxtext); return(BX_TOKEN_SYNC_CPU); }
+fast-forward    { bxlval.sval = strdup(bxtext); return(BX_TOKEN_FAST_FORWARD); }
+phy2log         { bxlval.sval = strdup(bxtext); return(BX_TOKEN_PHY_2_LOG); }
+addr-info       { bxlval.sval = strdup(bxtext); return(BX_TOKEN_INFO_ADDRESS); }
 ne2k            { bxlval.sval = strdup(bxtext); return(BX_TOKEN_NE2000); }
 ne2000          { bxlval.sval = strdup(bxtext); return(BX_TOKEN_NE2000); }
 page            { bxlval.sval = strdup(bxtext); return(BX_TOKEN_PAGE); }
@@ -155,6 +162,7 @@ ds              { bxlval.uval = BX_DBG_S
 fs              { bxlval.uval = BX_DBG_SREG_FS; return(BX_TOKEN_FS); }
 gs              { bxlval.uval = BX_DBG_SREG_GS; return(BX_TOKEN_GS); }
 flags|eflags    { bxlval.uval = 0; return (BX_TOKEN_FLAGS); }
+force-check     { bxlval.sval = strdup(bxtext); return(BX_TOKEN_ALWAYS_CHECK); }
 h|help          { bxlval.sval = strdup(bxtext); return(BX_TOKEN_HELP); }
 \?              |
 calc            { bxlval.sval = strdup(bxtext); return(BX_TOKEN_CALC); }
diff -uBbwNpr bochs-nocosim/bx_debug/linux.cc bochs/bx_debug/linux.cc
--- bochs-nocosim/bx_debug/linux.cc	2006-01-25 22:34:23.281250000 +0200
+++ bochs/bx_debug/linux.cc	2006-01-24 20:21:22.000000000 +0200
@@ -153,11 +153,11 @@ char *syscall_names_t::get_name (int n) 
 
 syscall_names_t syscall_names;
 
-void bx_dbg_linux_syscall (unsigned which_cpu)
-{
-  Bit32u eax = BX_CPU(which_cpu)->get_reg32(BX_32BIT_REG_EAX);
-  char *name = syscall_names.get_name (eax);
-  fprintf (stderr, "linux system call %s (#%d)\n", name, eax);
+void bx_dbg_linux_syscall () {
+  bx_dbg_cpu_t cpu;
+  bx_dbg_callback[0].get_cpu(&cpu);
+  char *name = syscall_names.get_name (cpu.eax);
+  fprintf (stderr, "linux system call %s (#%d)\n", name, cpu.eax);
 }
 
 #endif /* if BX_DEBUGGER */
diff -uBbwNpr bochs-nocosim/bx_debug/loader_misc.h bochs/bx_debug/loader_misc.h
--- bochs-nocosim/bx_debug/loader_misc.h	1970-01-01 02:00:00.000000000 +0200
+++ bochs/bx_debug/loader_misc.h	2003-11-28 17:07:25.000000000 +0200
@@ -0,0 +1,36 @@
+/////////////////////////////////////////////////////////////////////////
+// $Id: patch.cosimulation,v 1.2 2006-01-25 22:30:07 sshwarts Exp $
+/////////////////////////////////////////////////////////////////////////
+//
+//  Copyright (C) 2001  MandrakeSoft S.A.
+//
+//    MandrakeSoft S.A.
+//    43, rue d'Aboukir
+//    75002 Paris - France
+//    http://www.linux-mandrake.com/
+//    http://www.mandrakesoft.com/
+//
+//  This library is free software; you can redistribute it and/or
+//  modify it under the terms of the GNU Lesser General Public
+//  License as published by the Free Software Foundation; either
+//  version 2 of the License, or (at your option) any later version.
+//
+//  This library is distributed in the hope that it will be useful,
+//  but WITHOUT ANY WARRANTY; without even the implied warranty of
+//  MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
+//  Lesser General Public License for more details.
+//
+//  You should have received a copy of the GNU Lesser General Public
+//  License along with this library; if not, write to the Free Software
+//  Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA  02111-1307 USA
+
+typedef struct {
+  unsigned long dr0;
+  unsigned long dr1;
+  unsigned long dr2;
+  unsigned long dr3;
+  unsigned long dr6;
+  unsigned long dr7;
+  } bx_loader_misc_t;
+
+extern bx_loader_misc_t *bx_loader_misc_ptr;
diff -uBbwNpr bochs-nocosim/bx_debug/parser.y bochs/bx_debug/parser.y
--- bochs-nocosim/bx_debug/parser.y	2006-01-25 22:41:46.546875000 +0200
+++ bochs/bx_debug/parser.y	2006-01-25 20:13:44.000000000 +0200
@@ -113,6 +113,7 @@
 %token <sval> BX_TOKEN_STOP
 %token <sval> BX_TOKEN_RESET
 %token <sval> BX_TOKEN_PRINT
+%token <sval> BX_TOKEN_LOADER
 %token <sval> BX_TOKEN_STRING
 %token <sval> BX_TOKEN_DOIT
 %token <sval> BX_TOKEN_CRC
@@ -138,11 +139,18 @@
 %token <sval> BX_TOKEN_GLOBAL
 %token <sval> BX_TOKEN_WHERE
 %token <sval> BX_TOKEN_PRINT_STRING
+%token <sval> BX_TOKEN_DIFF_MEMORY
+%token <sval> BX_TOKEN_SYNC_MEMORY
+%token <sval> BX_TOKEN_SYNC_CPU
+%token <sval> BX_TOKEN_FAST_FORWARD
+%token <sval> BX_TOKEN_PHY_2_LOG
 %token <uval> BX_TOKEN_NUMERIC
 %token <ulval> BX_TOKEN_LONG_NUMERIC
+%token <sval> BX_TOKEN_INFO_ADDRESS
 %token <sval> BX_TOKEN_NE2000
 %token <sval> BX_TOKEN_PIC
 %token <sval> BX_TOKEN_PAGE
+%token <sval> BX_TOKEN_ALWAYS_CHECK
 %token <sval> BX_TOKEN_TRACEREGON
 %token <sval> BX_TOKEN_TRACEREGOFF
 %token <sval> BX_TOKEN_HELP
@@ -190,6 +198,7 @@ command:
     | set_cpu_command
     | disassemble_command
     | instrument_command
+    | loader_command
     | doit_command
     | crc_command
     | trace_on_command
@@ -205,6 +214,7 @@ command:
     | symbol_command
     | where_command
     | print_string_command
+    | cosim_commands
     | trace_reg_on_command
     | trace_reg_off_command
     | help_command
@@ -215,6 +225,48 @@ command:
       }
     ;
 
+cosim_commands:
+      BX_TOKEN_DIFF_MEMORY '\n'
+        {
+		bx_dbg_diff_memory();
+		free($1);
+	}
+    | BX_TOKEN_SYNC_MEMORY BX_TOKEN_ON  '\n'
+    | BX_TOKEN_SYNC_MEMORY BX_TOKEN_OFF '\n'
+        {
+		bx_dbg_sync_memory($2);
+		free($1);
+	}
+    | BX_TOKEN_SYNC_CPU BX_TOKEN_ON  '\n'
+    | BX_TOKEN_SYNC_CPU BX_TOKEN_OFF '\n'
+        {
+		bx_dbg_sync_cpu($2);
+		free($1);
+	}
+    | BX_TOKEN_FAST_FORWARD BX_TOKEN_NUMERIC '\n'
+        {
+		free($1);
+		bx_dbg_fast_forward($2);
+	}
+    | BX_TOKEN_PHY_2_LOG BX_TOKEN_NUMERIC '\n'
+        {
+		free($1);
+	}
+    | BX_TOKEN_INFO_ADDRESS BX_TOKEN_SEGREG ':' BX_TOKEN_NUMERIC '\n'
+        {
+		free($1);
+		bx_dbg_info_address($2, $4);
+        }
+    | BX_TOKEN_ALWAYS_CHECK BX_TOKEN_NUMERIC BX_TOKEN_ON '\n'
+        {
+		free($1);
+        }
+    | BX_TOKEN_ALWAYS_CHECK BX_TOKEN_NUMERIC BX_TOKEN_OFF '\n'
+        {
+		free($1);
+        }
+    ;
+
 BX_TOKEN_SEGREG:
       BX_TOKEN_CS
     | BX_TOKEN_ES
@@ -695,22 +747,44 @@ quit_command:
 examine_command:
       BX_TOKEN_EXAMINE BX_TOKEN_XFORMAT expression '\n'
         {
-        bx_dbg_examine_command($1, $2,1, $3, 1);
+        bx_dbg_examine_command($1, $2,1, $3,1, 0);
+#if BX_NUM_SIMULATORS >= 2
+        bx_dbg_examine_command($1, $2,1, $3,1, 1);
+#endif
         free($1); free($2);
         }
     | BX_TOKEN_EXAMINE BX_TOKEN_XFORMAT '\n'
         {
-        bx_dbg_examine_command($1, $2,1, 0, 0);
+        bx_dbg_examine_command($1, $2,1, 0,0, 0);
+#if BX_NUM_SIMULATORS >= 2
+        bx_dbg_examine_command($1, $2,1, 0,0, 1);
+#endif
         free($1); free($2);
         }
     | BX_TOKEN_EXAMINE expression '\n'
         {
-        bx_dbg_examine_command($1, NULL,0, $2, 1);
+        //FIXME HanishKVC This method of hunting thro all the 
+        //      simulators may be better than using 2 calls if 
+        //      BX_NUM_SIMULATORS greater than or equal to 2 as 
+        //      done for other cases of BX_TOKEN_EXAMINE
+        int iCurSim; 
+        for(iCurSim = 0; iCurSim < BX_NUM_SIMULATORS; iCurSim++)
+        {
+          bx_dbg_examine_command($1, NULL,0, $2,1, iCurSim);
+        }
         free($1);
         }
     | BX_TOKEN_EXAMINE '\n'
         {
-        bx_dbg_examine_command($1, NULL,0, 0, 0);
+        //FIXME HanishKVC This method of hunting thro all the 
+        //      simulators may be better than using 2 calls if 
+        //      BX_NUM_SIMULATORS greater than or equal to 2 as 
+        //      done for other cases of BX_TOKEN_EXAMINE
+        int iCurSim; 
+        for(iCurSim = 0; iCurSim < BX_NUM_SIMULATORS; iCurSim++)
+        {
+          bx_dbg_examine_command($1, NULL,0, 0,0, iCurSim);
+        }
         free($1);
         }
     ;
@@ -791,6 +865,14 @@ instrument_command:
         }
     ;
 
+loader_command:
+      BX_TOKEN_LOADER BX_TOKEN_STRING '\n'
+        {
+        bx_dbg_loader_command($2);
+        free($1); free($2);
+        }
+    ;
+
 doit_command:
       BX_TOKEN_DOIT BX_TOKEN_NUMERIC '\n'
         {
diff -uBbwNpr bochs-nocosim/bx_debug/sim2.cc bochs/bx_debug/sim2.cc
--- bochs-nocosim/bx_debug/sim2.cc	1970-01-01 02:00:00.000000000 +0200
+++ bochs/bx_debug/sim2.cc	2005-04-10 20:03:16.000000000 +0200
@@ -0,0 +1,199 @@
+/////////////////////////////////////////////////////////////////////////
+// $Id: patch.cosimulation,v 1.2 2006-01-25 22:30:07 sshwarts Exp $
+/////////////////////////////////////////////////////////////////////////
+//
+//  Copyright (C) 2001  MandrakeSoft S.A.
+//
+//    MandrakeSoft S.A.
+//    43, rue d'Aboukir
+//    75002 Paris - France
+//    http://www.linux-mandrake.com/
+//    http://www.mandrakesoft.com/
+//
+//  This library is free software; you can redistribute it and/or
+//  modify it under the terms of the GNU Lesser General Public
+//  License as published by the Free Software Foundation; either
+//  version 2 of the License, or (at your option) any later version.
+//
+//  This library is distributed in the hope that it will be useful,
+//  but WITHOUT ANY WARRANTY; without even the implied warranty of
+//  MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
+//  Lesser General Public License for more details.
+//
+//  You should have received a copy of the GNU Lesser General Public
+//  License along with this library; if not, write to the Free Software
+//  Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA  02111-1307 USA
+//
+/////////////////////////////////////////////////////////////////////////
+
+
+#include "bochs.h"
+
+
+// NOTE:  This file contains only stubs for a second CPU simulator
+//        to demonstrate use with the bochs debugger.  The goal is to
+//        be able to run multiple simulators in a co-simulation environment.
+//        Each simulator has it's own CPU and memory space.  There is only
+//        one set of device models, managed by the debugger.
+
+
+bx_bool  sim2_set_mem(Bit32u addr, unsigned len, Bit8u *buf);
+bx_bool  sim2_fetch_mem(Bit32u addr, unsigned len, Bit8u *buf);
+void     sim2_xlate_linear2phy(Bit32u linear, Bit32u *phy, bx_bool *valid);
+bx_bool  sim2_set_reg(unsigned reg, Bit32u val);
+Bit32u   sim2_get_reg(unsigned reg);
+bx_bool  sim2_set_cpu(bx_dbg_cpu_t *cpu);
+bx_bool  sim2_get_cpu(bx_dbg_cpu_t *cpu);
+unsigned       dirty_page_tbl_size;
+unsigned char sim2_dirty_pages[(BX_MAX_DIRTY_PAGE_TABLE_MEGS * 1024 * 1024) / 4096];
+void     sim2_atexit(void);
+unsigned sim2_query_pending(void);
+void     sim2_cpu_loop(void);
+void     sim2_take_irq(void);
+void     sim2_take_dma(void);
+void     sim2_reset_cpu(void);
+void     sim2_init_mem(int size_in_bytes);
+void     sim2_load_ROM(const char *path, Bit32u romaddress, Bit8u type);
+
+void     sim2_set_A20(unsigned val);
+void     sim2_set_NMI(unsigned val);
+void     sim2_set_RESET(unsigned val);
+void     sim2_set_INTR(unsigned val);
+void     sim2_force_interrupt(unsigned vector);
+
+#if BX_INSTRUMENTATION
+void     sim2_instr_start(void);
+void     sim2_instr_stop(void);
+void     sim2_instr_reset(void);
+void     sim2_instr_print(void);
+#endif
+#if BX_USE_LOADER
+void    sim2_loader(char *path);
+#endif
+
+
+#if BX_DBG_EXTENSIONS
+// return 0 if command not handled by extensions, bochs will handle
+// return 1 if command handled by extensions, bochs will ignore
+int bx_dbg_extensions(char *command)
+{
+  UNUSED(command);
+  return(0); // no extensions for now
+}
+#endif
+
+
+void sim2_init(bx_dbg_callback_t *callback, int argc, char *argv[])
+{
+  callback->setphymem           = sim2_set_mem;
+  callback->getphymem           = sim2_fetch_mem;
+  callback->xlate_linear2phy    = sim2_xlate_linear2phy;
+  callback->set_reg             = sim2_set_reg;
+  callback->get_reg             = sim2_get_reg;
+  callback->get_cpu             = sim2_get_cpu;
+  callback->set_cpu             = sim2_set_cpu;
+  callback->dirty_page_tbl_size = sizeof(sim2_dirty_pages);
+  callback->dirty_page_tbl      = sim2_dirty_pages;
+  callback->atexit              = sim2_atexit;
+  callback->query_pending       = sim2_query_pending;
+  callback->execute             = sim2_cpu_loop;
+  callback->take_irq            = sim2_take_irq;
+  callback->take_dma            = sim2_take_dma;
+  callback->reset_cpu           = sim2_reset_cpu;
+  callback->init_mem            = sim2_init_mem;
+  callback->load_ROM            = sim2_load_ROM;
+
+  // You may set this to NULL and use values in bx_pc_system as per
+  // docs-html/cosimulation.html
+  callback->set_A20             = sim2_set_A20;
+
+  callback->set_NMI             = sim2_set_NMI;
+  callback->set_RESET           = sim2_set_RESET;
+  callback->set_INTR            = sim2_set_INTR;
+  callback->force_interrupt     = sim2_force_interrupt;
+
+#if BX_INSTRUMENTATION
+  callback->instr_start         = sim2_instr_start;
+  callback->instr_stop          = sim2_instr_stop;
+  callback->instr_reset         = sim2_instr_reset;
+  callback->instr_print         = sim2_instr_print;
+#endif
+#if BX_USE_LOADER
+  callback->loader              = sim2_loader;
+#endif
+}
+
+bx_bool sim2_set_mem(Bit32u addr, unsigned len, Bit8u *buf)
+{
+  return(0);
+}
+
+bx_bool sim2_fetch_mem(Bit32u addr, unsigned len, Bit8u *buf)
+{
+  return(0);
+}
+
+void sim2_xlate_linear2phy(Bit32u linear, Bit32u *phy, bx_bool *valid) { }
+
+bx_bool sim2_set_reg(unsigned reg, Bit32u val)
+{
+  return(0);
+}
+
+Bit32u sim2_get_reg(unsigned reg)
+{
+  return(0);
+}
+
+bx_bool sim2_set_cpu(bx_dbg_cpu_t *cpu)
+{
+  return(0);
+}
+
+bx_bool sim2_get_cpu(bx_dbg_cpu_t *cpu)
+{
+  return(0);
+}
+
+void sim2_atexit(void) { }
+
+unsigned sim2_query_pending(void)
+{
+  return(0);
+}
+
+void sim2_cpu_loop(void) { }
+
+void sim2_take_irq(void) { }
+
+void sim2_take_dma(void) { }
+
+void sim2_reset_cpu(void) { }
+
+void sim2_init_mem(int size_in_bytes) { }
+
+void sim2_load_ROM(const char *path, Bit32u romaddress, Bit8u type) { }
+
+void sim2_set_A20(unsigned val) { }
+
+void sim2_set_NMI(unsigned val) { }
+
+void sim2_set_RESET(unsigned val) { }
+
+void sim2_set_INTR(unsigned val) { }
+
+void sim2_force_interrupt(unsigned vector) { }
+
+#if BX_INSTRUMENTATION
+void sim2_instr_start(void) { }
+
+void sim2_instr_stop(void) { }
+
+void sim2_instr_reset(void) { }
+
+void sim2_instr_print(void) { }
+#endif
+
+#if BX_USE_LOADER
+void sim2_loader(char *path) { }
+#endif
diff -uBbwNpr bochs-nocosim/config.h.in bochs/config.h.in
--- bochs-nocosim/config.h.in	2006-01-25 22:46:50.765625000 +0200
+++ bochs/config.h.in	2006-01-22 14:31:15.000000000 +0200
@@ -55,8 +55,10 @@
 #define BX_SUPPORT_SMP 0
 #define BX_BOOTSTRAP_PROCESSOR 0
 
-// Controls how many instances of BX_MEM_C are created. For
+// controls how many instances of BX_MEM_C are created.  For
 // SMP, use several processors with one shared memory space.
+// For cosimulation, you could use two processors and two address
+// spaces.
 #define BX_ADDRESS_SPACES 1
 
 #if BX_ADDRESS_SPACES != 1
@@ -685,6 +687,14 @@ typedef
 
 #define BX_INSTRUMENTATION    0
 
+#define BX_USE_LOADER    0
+
+// for debugger, CPU simulator handle ID
+//   0 is the default, for using only one CPU simulator
+//   1 is for the 2nd CPU simulator
+#define BX_SIM_ID    0
+#define BX_NUM_SIMULATORS 1
+
 // limited i440FX PCI support
 #define BX_SUPPORT_PCI 0
 
diff -uBbwNpr bochs-nocosim/configure.in bochs/configure.in
--- bochs-nocosim/configure.in	2006-01-25 22:37:48.781250000 +0200
+++ bochs/configure.in	2006-01-18 20:35:36.000000000 +0200
@@ -1392,6 +1392,34 @@ AC_ARG_ENABLE(instrumentation,
 AC_SUBST(INSTRUMENT_DIR)
 AC_SUBST(INSTRUMENT_VAR)
 
+AC_ARG_ENABLE(simid,
+  [  --enable-simid=0 or 1             CPU simulator ID if using more than one],
+  [if test "$enableval" = yes; then
+    AC_DEFINE(BX_SIM_ID, 0)
+   elif test "$enableval" = no; then
+    AC_DEFINE(BX_SIM_ID, 0)
+   else
+    AC_DEFINE_UNQUOTED(BX_SIM_ID, $enableval)
+   fi],
+  [
+    AC_DEFINE(BX_SIM_ID, 0)
+    ]
+  )
+
+AC_ARG_ENABLE(num-sim,
+  [  --enable-num-sim=1 or 2           number of CPU simulators],
+  [if test "$enableval" = yes; then
+    AC_DEFINE(BX_NUM_SIMULATORS, 1)
+   elif test "$enableval" = no; then
+    AC_DEFINE(BX_NUM_SIMULATORS, 1)
+   else
+    AC_DEFINE_UNQUOTED(BX_NUM_SIMULATORS, $enableval)
+   fi],
+  [
+    AC_DEFINE(BX_NUM_SIMULATORS, 1)
+    ]
+  )
+
 dnl // serial mode 'socket' needs wsock32.dll in non-plugin mode
 if test "$bx_plugins" = 0; then
   case $target in
diff -uBbwNpr bochs-nocosim/cpu/cpu.cc bochs/cpu/cpu.cc
--- bochs-nocosim/cpu/cpu.cc	2006-01-25 22:49:53.500000000 +0200
+++ bochs/cpu/cpu.cc	2006-01-24 21:07:45.000000000 +0200
@@ -1004,6 +1004,17 @@ bx_bool BX_CPU_C::dbg_is_end_instr_bpoin
     }
   }
 
+#if (BX_NUM_SIMULATORS >= 2)
+  // if async event pending, acknowlege them
+  if (bx_guard.async_changes_pending.which) {
+    if (bx_guard.async_changes_pending.which & BX_DBG_ASYNC_PENDING_A20)
+      bx_dbg_async_pin_ack(BX_DBG_ASYNC_PENDING_A20,
+                           bx_guard.async_changes_pending.a20);
+    if (bx_guard.async_changes_pending.which) {
+      BX_PANIC(("decode: async pending unrecognized."));
+    }
+  }
+#endif
   return(0); // no breakpoint
 }
 
diff -uBbwNpr bochs-nocosim/cpu/debugstuff.cc bochs/cpu/debugstuff.cc
--- bochs-nocosim/cpu/debugstuff.cc	2006-01-25 22:42:58.750000000 +0200
+++ bochs/cpu/debugstuff.cc	2006-01-25 20:13:44.000000000 +0200
@@ -987,6 +987,70 @@ bx_bool BX_CPU_C::dbg_set_cpu(bx_dbg_cpu
   return(1);
 }
 
+#if BX_SIM_ID == 0
+#  define BX_DBG_NULL_CALLBACK bx_dbg_null_callback0
+#else
+#  define BX_DBG_NULL_CALLBACK bx_dbg_null_callback1
+#endif
+void BX_DBG_NULL_CALLBACK(unsigned val)
+{
+  // bochs uses the pc_system variables, so this function is
+  // a stub for notification by the debugger, that a change
+  // occurred.
+  UNUSED(val);
+}
+
+  void
+#if BX_SIM_ID == 0
+bx_dbg_init_cpu_mem_env0(bx_dbg_callback_t *callback, int argc, char *argv[])
+#else
+bx_dbg_init_cpu_mem_env1(bx_dbg_callback_t *callback, int argc, char *argv[])
+#endif
+{
+  UNUSED(argc);
+  UNUSED(argv);
+
+#if 0
+#ifdef __GNUC__
+#warning hardcoding BX_CPU_THIS_PTR mem[0] and cpu[0]
+#endif
+  callback->setphymem           = BX_MEM(0)->dbg_set_mem;
+  callback->getphymem           = BX_MEM(0)->dbg_fetch_mem;
+  callback->xlate_linear2phy    = BX_CPU(0)->dbg_xlate_linear2phy;
+  callback->set_reg             = BX_CPU(0)->dbg_set_reg;
+  callback->get_reg             = BX_CPU(0)->dbg_get_reg;
+  callback->get_sreg            = BX_CPU(0)->dbg_get_sreg;
+  callback->get_cpu             = BX_CPU(0)->dbg_get_cpu;
+  callback->set_cpu             = BX_CPU(0)->dbg_set_cpu;
+  callback->dirty_page_tbl_size = sizeof(BX_MEM(0)->dbg_dirty_pages);
+  callback->dirty_page_tbl      = BX_MEM(0)->dbg_dirty_pages;
+  callback->atexit              = BX_CPU(0)->atexit;
+  callback->query_pending       = BX_CPU(0)->dbg_query_pending;
+  callback->execute             = BX_CPU(0)->cpu_loop;
+  callback->take_irq            = BX_CPU(0)->dbg_take_irq;
+  callback->take_dma            = BX_CPU(0)->dbg_take_dma;
+  callback->reset_cpu           = BX_CPU(0)->reset;
+  callback->init_mem            = BX_MEM(0)->init_memory;
+  callback->load_ROM            = BX_MEM(0)->load_ROM;
+  callback->set_A20             = NULL;
+  callback->set_NMI             = BX_DBG_NULL_CALLBACK;
+  callback->set_RESET           = BX_DBG_NULL_CALLBACK;
+  callback->set_INTR            = BX_CPU(0)->set_INTR;
+  callback->force_interrupt     = BX_CPU(0)->dbg_force_interrupt;
+
+#if BX_INSTRUMENTATION
+  callback->instr_start         = bx_instr_start;
+  callback->instr_stop          = bx_instr_stop;
+  callback->instr_reset         = bx_instr_reset;
+  callback->instr_print         = bx_instr_print;
+#endif
+#if BX_USE_LOADER
+  callback->loader              = bx_dbg_loader;
+#endif
+  callback->crc32               = BX_MEM(0)->dbg_crc32;
+#endif
+}
+
 #endif  // #if BX_DEBUGGER
 
 void BX_CPU_C::atexit(void)
diff -uBbwNpr bochs-nocosim/cpu/exception.cc bochs/cpu/exception.cc
--- bochs-nocosim/cpu/exception.cc	2006-01-25 22:34:50.328125000 +0200
+++ bochs/cpu/exception.cc	2005-12-13 00:01:22.000000000 +0200
@@ -769,7 +769,7 @@ void BX_CPU_C::interrupt(Bit8u vector, b
   BX_CPU_THIS_PTR show_flag |= Flag_intsig;
 #if BX_DEBUG_LINUX
   if (bx_dbg.linux_syscall) {
-    if (vector == 0x80) bx_dbg_linux_syscall(BX_CPU_ID);
+    if (vector == 0x80) bx_dbg_linux_syscall ();
   }
 #endif
 #endif
diff -uBbwNpr bochs-nocosim/cpu/init.cc bochs/cpu/init.cc
--- bochs-nocosim/cpu/init.cc	2006-01-25 22:43:37.546875000 +0200
+++ bochs/cpu/init.cc	2006-01-24 21:03:54.000000000 +0200
@@ -942,7 +942,7 @@ void BX_CPU_C::sanity_checks(void)
   if (sizeof(Bit64u) != 8  ||  sizeof(Bit64s) != 8)
     BX_PANIC(("data type Bit64u or Bit64u is not of length 8 bytes!"));
 
-  BX_DEBUG(("#(%u)all sanity checks passed!", BX_CPU_ID));
+  BX_DEBUG(( "#(%u)all sanity checks passed!", BX_SIM_ID ));
 }
 
 
diff -uBbwNpr bochs-nocosim/cpu/lazy_flags.cc bochs/cpu/lazy_flags.cc
--- bochs-nocosim/cpu/lazy_flags.cc	2006-01-25 22:43:53.859375000 +0200
+++ bochs/cpu/lazy_flags.cc	2005-10-20 19:33:36.000000000 +0200
@@ -30,6 +30,7 @@
 #include "bochs.h"
 #define LOG_THIS BX_CPU_THIS_PTR
 
+#if BX_SIM_ID == 0   // only need to define once
 // This array defines a look-up table for the even parity-ness
 // of an 8bit quantity, for optimal assignment of the parity bit
 // in the EFLAGS register
@@ -51,6 +52,7 @@ const bx_bool bx_parity_lookup[256] = {
   0, 1, 1, 0, 1, 0, 0, 1, 1, 0, 0, 1, 0, 1, 1, 0,
   1, 0, 0, 1, 0, 1, 1, 0, 0, 1, 1, 0, 1, 0, 0, 1
 };
+#endif
 
 bx_bool BX_CPU_C::get_CFLazy(void)
 {
diff -uBbwNpr bochs-nocosim/load32bitOShack.cc bochs/load32bitOShack.cc
--- bochs-nocosim/load32bitOShack.cc	2006-01-25 22:44:29.515625000 +0200
+++ bochs/load32bitOShack.cc	2005-11-09 19:17:06.000000000 +0200
@@ -309,8 +309,10 @@ bx_load_kernel_image(char *path, Bit32u 
     offset += ret;
     }
   close(fd);
-  BX_INFO(("load_kernel_image: '%s', size=%u read into memory at %08x",
-       path, (unsigned) stat_buf.st_size, (unsigned) paddr));
+  BX_INFO(( "#(%u) load_kernel_image: '%s', size=%u read into memory at %08x",
+          BX_SIM_ID, path,
+          (unsigned) stat_buf.st_size,
+          (unsigned) paddr ));
 
   return page_size;
 }
diff -uBbwNpr bochs-nocosim/memory/misc_mem.cc bochs/memory/misc_mem.cc
--- bochs-nocosim/memory/misc_mem.cc	2006-01-25 22:45:37.656250000 +0200
+++ bochs/memory/misc_mem.cc	2006-01-24 21:03:55.000000000 +0200
@@ -40,7 +40,7 @@ Bit32u BX_MEM_C::get_memory_in_k(void)
 BX_MEM_C::BX_MEM_C(void)
 {
   char mem[6];
-  snprintf(mem, 6, "MEM0");
+  snprintf(mem, 6, "MEM%d", BX_SIM_ID);
   put(mem);
   settype(MEMLOG);
 
@@ -85,7 +85,7 @@ BX_MEM_C::~BX_MEM_C(void)
     memory_handlers = NULL;
   }
   else {
-    BX_DEBUG(("Memory not freed as it wasn't allocated !"));
+    BX_DEBUG(("(%u)   memory not freed as it wasn't allocated!", BX_SIM_ID));
   }
 }
 
diff -uBbwNpr bochs-nocosim/pc_system.cc bochs/pc_system.cc
--- bochs-nocosim/pc_system.cc	2006-01-25 22:50:16.625000000 +0200
+++ bochs/pc_system.cc	2006-01-20 21:12:03.000000000 +0200
@@ -104,12 +104,15 @@ void bx_pc_system_c::set_HRQ(bx_bool val
     BX_CPU(0)->async_event = 1;
 }
 
+
+#if (BX_NUM_SIMULATORS < 2)
 void bx_pc_system_c::set_INTR(bx_bool value)
 {
   if (bx_dbg.interrupts)
     BX_INFO(("pc_system: Setting INTR=%d on bootstrap processor %d", (int)value, BX_BOOTSTRAP_PROCESSOR));
   BX_CPU(BX_BOOTSTRAP_PROCESSOR)->set_INTR(value);
 }
+#endif
 
 //
 // Read from the IO memory address space
