// -*- mode:c++ -*-

// Copyright (c) 2007 MIPS Technologies, Inc.
// All rights reserved.
//
// Redistribution and use in source and binary forms, with or without
// modification, are permitted provided that the following conditions are
// met: redistributions of source code must retain the above copyright
// notice, this list of conditions and the following disclaimer;
// redistributions in binary form must reproduce the above copyright
// notice, this list of conditions and the following disclaimer in the
// documentation and/or other materials provided with the distribution;
// neither the name of the copyright holders nor the names of its
// contributors may be used to endorse or promote products derived from
// this software without specific prior written permission.
//
// THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
// "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
// LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
// A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
// OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
// SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
// LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
// DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
// THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
// (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
// OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
//
// Authors: Korey Sewell
//          Jaidev Patwardhan

def operand_types {{
    'sb' : 'int8_t',
    'ub' : 'uint8_t',
    'sh' : 'int16_t',
    'uh' : 'uint16_t',
    'sw' : 'int32_t',
    'uw' : 'uint32_t',
    'sd' : 'int64_t',
    'ud' : 'uint64_t',
    'sf' : 'float',
    'df' : 'double'
}};

def operands {{
    #General Purpose Integer Reg Operands
    'Rd': ('IntReg', 'uw', 'RD', 'IsInteger', 1),
    'Rs': ('IntReg', 'uw', 'RS', 'IsInteger', 2),
    'Rt': ('IntReg', 'uw', 'RT', 'IsInteger', 3),

    #Immediate Value operand
    'IntImm': ('IntReg', 'uw', 'INTIMM', 'IsInteger', 3),

    #Operands used for Link or Syscall Insts
    'R31': ('IntReg', 'uw','31','IsInteger', 4),
    'R2':  ('IntReg', 'uw','2', 'IsInteger', 5),

    #Special Integer Reg operands
    'LO0':  ('IntReg', 'uw','INTREG_LO', 'IsInteger', 6),
    'HI0':  ('IntReg', 'uw','INTREG_HI', 'IsInteger', 7),

    #Bitfield-dependent HI/LO Register Access
    'LO_RD_SEL': ('IntReg','uw','INTREG_DSP_LO0 + ACDST*3', None, 6),
    'HI_RD_SEL': ('IntReg','uw','INTREG_DSP_HI0 + ACDST*3', None, 7),
    'LO_RS_SEL': ('IntReg','uw','INTREG_DSP_LO0 + ACSRC*3', None, 6),
    'HI_RS_SEL': ('IntReg','uw','INTREG_DSP_HI0 + ACSRC*3', None, 7),

    #DSP Special Purpose Integer Operands
    'DSPControl': ('IntReg', 'uw', 'INTREG_DSP_CONTROL', None, 8),
    'DSPLo0': ('IntReg', 'uw', 'INTREG_LO', None, 1),
    'DSPHi0': ('IntReg', 'uw', 'INTREG_HI', None, 1),
    'DSPACX0': ('IntReg', 'uw', 'INTREG_DSP_ACX0', None, 1),
    'DSPLo1': ('IntReg', 'uw', 'INTREG_DSP_LO1', None, 1),
    'DSPHi1': ('IntReg', 'uw', 'INTREG_DSP_HI1', None, 1),
    'DSPACX1': ('IntReg', 'uw', 'INTREG_DSP_ACX1', None, 1),
    'DSPLo2': ('IntReg', 'uw', 'INTREG_DSP_LO2', None, 1),
    'DSPHi2': ('IntReg', 'uw', 'INTREG_DSP_HI2', None, 1),
    'DSPACX2': ('IntReg', 'uw', 'INTREG_DSP_ACX2', None, 1),
    'DSPLo3': ('IntReg', 'uw', 'INTREG_DSP_LO3', None, 1),
    'DSPHi3': ('IntReg', 'uw', 'INTREG_DSP_HI3', None, 1),
    'DSPACX3': ('IntReg', 'uw', 'INTREG_DSP_ACX3', None, 1),

    #Floating Point Reg Operands
    'Fd': ('FloatReg', 'sf', 'FD', 'IsFloating', 1),
    'Fs': ('FloatReg', 'sf', 'FS', 'IsFloating', 2),
    'Ft': ('FloatReg', 'sf', 'FT', 'IsFloating', 3),
    'Fr': ('FloatReg', 'sf', 'FR', 'IsFloating', 3),

    #Special Purpose Floating Point Control Reg Operands
    'FIR':  ('FloatReg', 'uw', 'FLOATREG_FIR', 'IsFloating', 1),
    'FCCR': ('FloatReg', 'uw', 'FLOATREG_FCCR', 'IsFloating', 2),
    'FEXR': ('FloatReg', 'uw', 'FLOATREG_FEXR', 'IsFloating', 3),
    'FENR': ('FloatReg', 'uw', 'FLOATREG_FENR', 'IsFloating', 3),
    'FCSR': ('FloatReg', 'uw', 'FLOATREG_FCSR', 'IsFloating', 3),

    #Operands For Paired Singles FP Operations
    'Fd1': ('FloatReg', 'sf', 'FD', 'IsFloating', 4),
    'Fd2': ('FloatReg', 'sf', 'FD+1', 'IsFloating', 4),
    'Fs1': ('FloatReg', 'sf', 'FS', 'IsFloating', 5),
    'Fs2': ('FloatReg', 'sf', 'FS+1', 'IsFloating', 5),
    'Ft1': ('FloatReg', 'sf', 'FT', 'IsFloating', 6),
    'Ft2': ('FloatReg', 'sf', 'FT+1', 'IsFloating', 6),
    'Fr1': ('FloatReg', 'sf', 'FR', 'IsFloating', 7),
    'Fr2': ('FloatReg', 'sf', 'FR+1', 'IsFloating', 7),

    #Status Control Reg
    'Status': ('ControlReg', 'uw', 'MISCREG_STATUS', None, 1),

    #LL Flag
    'LLFlag': ('ControlReg', 'uw', 'MISCREG_LLFLAG', None, 1),

    #Thread pointer value for SE mode
    'TpValue': ('ControlReg', 'ud', 'MISCREG_TP_VALUE', None, 1),

    # Index Register
    'Index': ('ControlReg','uw','MISCREG_INDEX',None,1),


    'CP0_RD_SEL': ('ControlReg', 'uw', '(RD << 3 | SEL)', None, 1),

    #MT Control Regs
    'MVPConf0': ('ControlReg', 'uw', 'MISCREG_MVP_CONF0', None, 1),
    'MVPControl': ('ControlReg', 'uw', 'MISCREG_MVP_CONTROL', None, 1),
    'TCBind': ('ControlReg', 'uw', 'MISCREG_TC_BIND', None, 1),
    'TCStatus': ('ControlReg', 'uw', 'MISCREG_TC_STATUS', None, 1),
    'TCRestart': ('ControlReg', 'uw', 'MISCREG_TC_RESTART', None, 1),
    'VPEConf0': ('ControlReg', 'uw', 'MISCREG_VPE_CONF0', None, 1),
    'VPEControl': ('ControlReg', 'uw', 'MISCREG_VPE_CONTROL', None, 1),
    'YQMask': ('ControlReg', 'uw', 'MISCREG_YQMASK', None, 1),

    #CP0 Control Regs
    'EntryHi': ('ControlReg','uw', 'MISCREG_ENTRYHI',None,1),
    'EntryLo0': ('ControlReg','uw', 'MISCREG_ENTRYLO0',None,1),
    'EntryLo1': ('ControlReg','uw', 'MISCREG_ENTRYLO1',None,1),
    'PageMask': ('ControlReg','uw', 'MISCREG_PAGEMASK',None,1),
    'Random': ('ControlReg','uw', 'MISCREG_CP0_RANDOM',None,1),
    'ErrorEPC': ('ControlReg','uw', 'MISCREG_ERROR_EPC',None,1),
    'EPC': ('ControlReg','uw', 'MISCREG_EPC',None,1),
    'DEPC': ('ControlReg','uw', 'MISCREG_DEPC',None,1),
    'IntCtl': ('ControlReg','uw', 'MISCREG_INTCTL',None,1),
    'SRSCtl': ('ControlReg','uw', 'MISCREG_SRSCTL',None,1),
    'Config': ('ControlReg','uw', 'MISCREG_CONFIG',None,1),
    'Config3': ('ControlReg','uw', 'MISCREG_CONFIG3',None,1),
    'Config1': ('ControlReg','uw', 'MISCREG_CONFIG1',None,1),
    'Config2': ('ControlReg','uw', 'MISCREG_CONFIG2',None,1),
    'PageGrain': ('ControlReg','uw', 'MISCREG_PAGEGRAIN',None,1),
    'Debug': ('ControlReg','uw', 'MISCREG_DEBUG',None,1),
    'Cause': ('ControlReg','uw', 'MISCREG_CAUSE',None,1),

    #Memory Operand
    'Mem': ('Mem', 'uw', None, ('IsMemRef', 'IsLoad', 'IsStore'), 4),

    #Program Counter Operands
    'PC': ('PCState', 'uw', 'pc', (None, None, 'IsControl'), 4),
    'NPC': ('PCState', 'uw', 'npc', (None, None, 'IsControl'), 4),
    'NNPC': ('PCState', 'uw', 'nnpc', (None, None, 'IsControl'), 4)
}};
