// -*- mode:c++ -*-

// Copyright (c) 2010 ARM Limited
// All rights reserved
//
// The license below extends only to copyright in the software and shall
// not be construed as granting a license to any other intellectual
// property including but not limited to intellectual property relating
// to a hardware implementation of the functionality of the software
// licensed hereunder.  You may use the software subject to the license
// terms below provided that you ensure that this notice is replicated
// unmodified and in its entirety in all distributions of the software,
// modified or unmodified, in source code or in binary form.
//
// Redistribution and use in source and binary forms, with or without
// modification, are permitted provided that the following conditions are
// met: redistributions of source code must retain the above copyright
// notice, this list of conditions and the following disclaimer;
// redistributions in binary form must reproduce the above copyright
// notice, this list of conditions and the following disclaimer in the
// documentation and/or other materials provided with the distribution;
// neither the name of the copyright holders nor the names of its
// contributors may be used to endorse or promote products derived from
// this software without specific prior written permission.
//
// THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
// "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
// LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
// A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
// OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
// SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
// LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
// DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
// THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
// (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
// OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
//
// Authors: Gabe Black

let {{

    header_output = ""
    decoder_output = ""
    exec_output = ""

    calcGECode = '''
        CondCodesGE = resTemp;
    '''

    calcQCode = '''
        CpsrQ = (resTemp & 1) << 27;
    '''

    def createCcCode(negBit, carry, overflow):
        code = ""
        code += '''
            uint16_t _iz, _in;
            _in = (resTemp >> %d) & 1;
            _iz = (resTemp == 0);
            CondCodesNZ = (_in << 1) | _iz;
            DPRINTF(Arm, "(in, iz) = (%%d, %%d)\\n", _in, _iz);
        ''' % negBit
        if overflow and overflow != "none":
            code +=  '''
                uint16_t _iv;
                _iv = %s & 1;
                CondCodesV =  _iv;
                DPRINTF(Arm, "(iv) = (%%d)\\n", _iv);
            ''' % overflow
        if carry and carry != "none":
            code += '''
                uint16_t _ic;
                _ic = %s & 1;
                CondCodesC =  _ic;
                DPRINTF(Arm, "(ic) = (%%d)\\n", _ic);
            ''' % carry
        return code

    # Dict of code to set the carry flag. (imm, reg, reg-reg)
    oldC = 'CondCodesC'
    carryCode = {
        "none": ("none", "none", "none"),
        "llbit": ("none", "none", "none"),
        "saturate": ('0', '0', '0'),
        "overflow": ('0', '0', '0'),
        "ge": ('0', '0', '0'),
        "add": ('findCarry(32, resTemp, Op1, secondOp)',
                'findCarry(32, resTemp, Op1, secondOp)',
                'findCarry(32, resTemp, Op1, secondOp)'),
        "sub": ('findCarry(32, resTemp, Op1, ~secondOp)',
                'findCarry(32, resTemp, Op1, ~secondOp)',
                'findCarry(32, resTemp, Op1, ~secondOp)'),
        "rsb": ('findCarry(32, resTemp, secondOp, ~Op1)',
                'findCarry(32, resTemp, secondOp, ~Op1)',
                'findCarry(32, resTemp, secondOp, ~Op1)'),
        "logic": ('(rotC ? bits(secondOp, 31) : %s)' % oldC,
                  'shift_carry_imm(Op2, shiftAmt, shiftType, %s)' % oldC,
                  'shift_carry_rs(Op2, Shift<7:0>, shiftType, %s)' % oldC)
    }
    # Dict of code to set the overflow flag.
    overflowCode = {
        "none": "none",
        "llbit": "none",
        "saturate": '0',
        "overflow": '0',
        "ge": '0',
        "add": 'findOverflow(32, resTemp, Op1, secondOp)',
        "sub": 'findOverflow(32, resTemp, Op1, ~secondOp)',
        "rsb": 'findOverflow(32, resTemp, secondOp, ~Op1)',
        "logic": "none"
    }

    secondOpRe = re.compile("secondOp")
    immOp2 = "imm"
    regOp2 = "shift_rm_imm(Op2, shiftAmt, shiftType, OptShiftRmCondCodesC)"
    regRegOp2 = "shift_rm_rs(Op2, Shift<7:0>, shiftType, 0)"

    def buildImmDataInst(mnem, code, flagType = "logic", suffix = "Imm", \
                         buildCc = True, buildNonCc = True, instFlags = []):
        cCode = carryCode[flagType]
        vCode = overflowCode[flagType]
        negBit = 31
        if flagType == "llbit":
            negBit = 63
        if flagType == "saturate":
            immCcCode = calcQCode
        elif flagType == "ge":
            immCcCode = calcGECode
        else:
            immCcCode = createCcCode(negBit, secondOpRe.sub(immOp2, cCode[0]),
                                     secondOpRe.sub(immOp2, vCode))

        immCode = secondOpRe.sub(immOp2, code)
        immIop = InstObjParams(mnem, mnem.capitalize() + suffix, "DataImmOp",
                       {"code" : immCode,
                        "predicate_test": pickPredicate(immCode)}, instFlags)
        immIopCc = InstObjParams(mnem + "s", mnem.capitalize() + suffix + "Cc",
             "DataImmOp",
             {"code" : immCode + immCcCode,
              "predicate_test": pickPredicate(immCode + immCcCode)}, instFlags)

        def subst(iop):
            global header_output, decoder_output, exec_output
            header_output += DataImmDeclare.subst(iop)
            decoder_output += DataImmConstructor.subst(iop)
            exec_output += PredOpExecute.subst(iop)

        if buildNonCc:
            subst(immIop)
        if buildCc:
            subst(immIopCc)

    def buildRegDataInst(mnem, code, flagType = "logic", suffix = "Reg", \
                         buildCc = True, buildNonCc = True, isRasPop = "0", \
                         isBranch = "0", instFlags = []):
        cCode = carryCode[flagType]
        vCode = overflowCode[flagType]
        negBit = 31
        regCcCode = ""
        if flagType == "llbit":
            negBit = 63
        if flagType == "saturate":
            regCcCode = calcQCode
        elif flagType == "ge":
            regCcCode = calcGECode
        else:
            regCcCode = createCcCode(negBit,secondOpRe.sub(regOp2, cCode[1]),
                                     secondOpRe.sub(regOp2, vCode))

        regCode = secondOpRe.sub(regOp2, code)

        # If we end up needing CondCodesC then remove any trace of the OptShift
        if re.search('(?<!OptShiftRm)CondCodesC(?!.*=)', regCode + regCcCode):
            regCode = re.sub('OptShiftRmCondCodesC', 'CondCodesC', regCode)
            regCcCode = re.sub('OptShiftRmCondCodesC', 'CondCodesC', regCcCode)

        regIop = InstObjParams(mnem, mnem.capitalize() + suffix, "DataRegOp",
                       {"code" : regCode, "is_ras_pop" : isRasPop,
                        "is_branch" : isBranch,
                        "predicate_test": pickPredicate(regCode)}, instFlags)
        regIopCc = InstObjParams(mnem + "s", mnem.capitalize() + suffix + "Cc",
                         "DataRegOp",
                         {"code" : regCode + regCcCode,
                          "predicate_test": pickPredicate(regCode + regCcCode),
                          "is_ras_pop" : isRasPop,
                          "is_branch" : isBranch}, instFlags)

        def subst(iop):
            global header_output, decoder_output, exec_output
            header_output += DataRegDeclare.subst(iop)
            decoder_output += DataRegConstructor.subst(iop)
            exec_output += PredOpExecute.subst(iop)

        if buildNonCc:
            subst(regIop)
        if buildCc:
            subst(regIopCc)

    def buildRegRegDataInst(mnem, code, flagType = "logic", \
                            suffix = "RegReg", \
                            buildCc = True, buildNonCc = True):
        cCode = carryCode[flagType]
        vCode = overflowCode[flagType]
        negBit = 31
        if flagType == "llbit":
            negBit = 63
        if flagType == "saturate":
            regRegCcCode = calcQCode
        elif flagType == "ge":
            regRegCcCode = calcGECode
        else:
            regRegCcCode = createCcCode(negBit,
                                        secondOpRe.sub(regRegOp2, cCode[2]),
                                        secondOpRe.sub(regRegOp2, vCode))

        regRegCode = secondOpRe.sub(regRegOp2, code)
        regRegIop = InstObjParams(mnem, mnem.capitalize() + suffix,
                          "DataRegRegOp",
                          {"code" : regRegCode,
                           "predicate_test": pickPredicate(regRegCode)})
        regRegIopCc = InstObjParams(mnem + "s",
                mnem.capitalize() + suffix + "Cc",
                "DataRegRegOp",
                {"code" : regRegCode + regRegCcCode,
                 "predicate_test": pickPredicate(regRegCode + regRegCcCode)})

        def subst(iop):
            global header_output, decoder_output, exec_output
            header_output += DataRegRegDeclare.subst(iop)
            decoder_output += DataRegRegConstructor.subst(iop)
            exec_output += PredOpExecute.subst(iop)

        if buildNonCc:
            subst(regRegIop)
        if buildCc:
            subst(regRegIopCc)

    def buildDataInst(mnem, code, flagType = "logic", \
                      aiw = True, regRegAiw = True,
                      subsPcLr = True, isRasPop = "0", isBranch = "0"):
        regRegCode = instCode = code
        if aiw:
            instCode = "AIW" + instCode
            if regRegAiw:
                regRegCode = "AIW" + regRegCode

        buildImmDataInst(mnem, instCode, flagType)
        buildRegDataInst(mnem, instCode, flagType,
                         isRasPop = isRasPop, isBranch = isBranch)
        buildRegRegDataInst(mnem, regRegCode, flagType)
        if subsPcLr:
            code += '''
            SCTLR sctlr = Sctlr;
            CPSR old_cpsr = Cpsr;

            CPSR new_cpsr =
                cpsrWriteByInstr(old_cpsr, Spsr, 0xF, true, sctlr.nmfi);
            Cpsr = ~CondCodesMask & new_cpsr;
            CondCodesNZ = new_cpsr.nz;
            CondCodesC = new_cpsr.c;
            CondCodesV = new_cpsr.v;
            CondCodesGE = new_cpsr.ge;

            NextThumb = (new_cpsr).t;
            NextJazelle = (new_cpsr).j;
            NextItState = (((new_cpsr).it2 << 2) & 0xFC)
                | ((new_cpsr).it1 & 0x3);
            SevMailbox = 1;
            '''
            buildImmDataInst(mnem + 's', code, flagType,
                             suffix = "ImmPclr", buildCc = False,
                             instFlags = ["IsSerializeAfter","IsNonSpeculative"])
            buildRegDataInst(mnem + 's', code, flagType,
                             suffix = "RegPclr", buildCc = False,
                             instFlags = ["IsSerializeAfter","IsNonSpeculative"])

    buildDataInst("and", "Dest = resTemp = Op1 & secondOp;")
    buildDataInst("eor", "Dest = resTemp = Op1 ^ secondOp;")
    buildDataInst("sub", "Dest = resTemp = Op1 - secondOp;", "sub")
    buildDataInst("rsb", "Dest = resTemp = secondOp - Op1;", "rsb")
    buildDataInst("add", "Dest = resTemp = Op1 + secondOp;", "add")
    buildImmDataInst("adr", '''
                               Dest = resTemp = (PC & ~0x3) +
                               (op1 ? secondOp : -secondOp);
                            ''')
    buildDataInst("adc", "Dest = resTemp = Op1 + secondOp + %s;" % oldC, "add")
    buildDataInst("sbc", "Dest = resTemp = Op1 - secondOp - !%s;" % oldC, "sub")
    buildDataInst("rsc", "Dest = resTemp = secondOp - Op1 - !%s;" % oldC, "rsb")
    buildDataInst("tst", "resTemp = Op1 & secondOp;", aiw = False)
    buildDataInst("teq", "resTemp = Op1 ^ secondOp;", aiw = False)
    buildDataInst("cmp", "resTemp = Op1 - secondOp;", "sub", aiw = False)
    buildDataInst("cmn", "resTemp = Op1 + secondOp;", "add", aiw = False)
    buildDataInst("orr", "Dest = resTemp = Op1 | secondOp;")
    buildDataInst("orn", "Dest = resTemp = Op1 | ~secondOp;", aiw = False)
    buildDataInst("mov", "Dest = resTemp = secondOp;", regRegAiw = False,
                  isRasPop = "op1 == INTREG_LR", isBranch = "dest == INTREG_PC")
    buildDataInst("bic", "Dest = resTemp = Op1 & ~secondOp;")
    buildDataInst("mvn", "Dest = resTemp = ~secondOp;")
    buildDataInst("movt",
                  "Dest = resTemp = insertBits(Op1, 31, 16, secondOp);",
                  aiw = False)

    buildRegDataInst("qadd", '''
            int32_t midRes;
            resTemp = saturateOp<32>(midRes, Op1_sw, Op2_sw);
                                     Dest = midRes;
        ''', flagType="saturate", buildNonCc=False)
    buildRegDataInst("qadd16", '''
            int32_t midRes;
            for (unsigned i = 0; i < 2; i++) {
                int high = (i + 1) * 16 - 1;
                int low = i * 16;
                int64_t arg1 = sext<16>(bits(Op1_sw, high, low));
                int64_t arg2 = sext<16>(bits(Op2_sw, high, low));
                saturateOp<16>(midRes, arg1, arg2);
                replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("qadd8", '''
            int32_t midRes;
            for (unsigned i = 0; i < 4; i++) {
                int high = (i + 1) * 8 - 1;
                int low = i * 8;
                int64_t arg1 = sext<8>(bits(Op1_sw, high, low));
                int64_t arg2 = sext<8>(bits(Op2_sw, high, low));
                saturateOp<8>(midRes, arg1, arg2);
                replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("qdadd", '''
            int32_t midRes;
            resTemp = saturateOp<32>(midRes, Op2_sw, Op2_sw) |
                      saturateOp<32>(midRes, Op1_sw, midRes);
            Dest = midRes;
        ''', flagType="saturate", buildNonCc=False)
    buildRegDataInst("qsub", '''
            int32_t midRes;
            resTemp = saturateOp<32>(midRes, Op1_sw, Op2_sw, true);
            Dest = midRes;
        ''', flagType="saturate")
    buildRegDataInst("qsub16", '''
            int32_t midRes;
            for (unsigned i = 0; i < 2; i++) {
                 int high = (i + 1) * 16 - 1;
                 int low = i * 16;
                 int64_t arg1 = sext<16>(bits(Op1_sw, high, low));
                 int64_t arg2 = sext<16>(bits(Op2_sw, high, low));
                 saturateOp<16>(midRes, arg1, arg2, true);
                 replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("qsub8", '''
            int32_t midRes;
            for (unsigned i = 0; i < 4; i++) {
                 int high = (i + 1) * 8 - 1;
                 int low = i * 8;
                 int64_t arg1 = sext<8>(bits(Op1_sw, high, low));
                 int64_t arg2 = sext<8>(bits(Op2_sw, high, low));
                 saturateOp<8>(midRes, arg1, arg2, true);
                 replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("qdsub", '''
            int32_t midRes;
            resTemp = saturateOp<32>(midRes, Op2_sw, Op2_sw) |
                      saturateOp<32>(midRes, Op1_sw, midRes, true);
            Dest = midRes;
        ''', flagType="saturate", buildNonCc=False)
    buildRegDataInst("qasx", '''
            int32_t midRes;
            int64_t arg1Low = sext<16>(bits(Op1_sw, 15, 0));
            int64_t arg1High = sext<16>(bits(Op1_sw, 31, 16));
            int64_t arg2Low = sext<16>(bits(Op2_sw, 15, 0));
            int64_t arg2High = sext<16>(bits(Op2_sw, 31, 16));
            saturateOp<16>(midRes, arg1Low, arg2High, true);
            replaceBits(resTemp, 15, 0, midRes);
            saturateOp<16>(midRes, arg1High, arg2Low);
            replaceBits(resTemp, 31, 16, midRes);
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("qsax", '''
            int32_t midRes;
            int64_t arg1Low = sext<16>(bits(Op1_sw, 15, 0));
            int64_t arg1High = sext<16>(bits(Op1_sw, 31, 16));
            int64_t arg2Low = sext<16>(bits(Op2_sw, 15, 0));
            int64_t arg2High = sext<16>(bits(Op2_sw, 31, 16));
            saturateOp<16>(midRes, arg1Low, arg2High);
            replaceBits(resTemp, 15, 0, midRes);
            saturateOp<16>(midRes, arg1High, arg2Low, true);
            replaceBits(resTemp, 31, 16, midRes);
            Dest = resTemp;
        ''', flagType="none", buildCc=False)

    buildRegDataInst("sadd8", '''
            uint32_t geBits = 0;
            resTemp = 0;
            for (unsigned i = 0; i < 4; i++) {
                int high = (i + 1) * 8 - 1;
                int low = i * 8;
                int32_t midRes = sext<8>(bits(Op1_sw, high, low)) +
                                 sext<8>(bits(Op2_sw, high, low));
                replaceBits(resTemp, high, low, midRes);
                if (midRes >= 0) {
                    geBits = geBits | (1 << i);
                }
            }
            Dest = resTemp;
            resTemp = geBits;
        ''', flagType="ge", buildNonCc=False)
    buildRegDataInst("sadd16", '''
            uint32_t geBits = 0;
            resTemp = 0;
            for (unsigned i = 0; i < 2; i++) {
                int high = (i + 1) * 16 - 1;
                int low = i * 16;
                int32_t midRes = sext<16>(bits(Op1_sw, high, low)) +
                                 sext<16>(bits(Op2_sw, high, low));
                replaceBits(resTemp, high, low, midRes);
                if (midRes >= 0) {
                    geBits = geBits | (0x3 << (i * 2));
                }
            }
            Dest = resTemp;
            resTemp = geBits;
        ''', flagType="ge", buildNonCc=False)

    buildRegDataInst("ssub8", '''
            uint32_t geBits = 0;
            resTemp = 0;
            for (unsigned i = 0; i < 4; i++) {
                int high = (i + 1) * 8 - 1;
                int low = i * 8;
                int32_t midRes = sext<8>(bits(Op1_sw, high, low)) -
                                 sext<8>(bits(Op2_sw, high, low));
                replaceBits(resTemp, high, low, midRes);
                if (midRes >= 0) {
                    geBits = geBits | (1 << i);
                }
            }
            Dest = resTemp;
            resTemp = geBits;
        ''', flagType="ge", buildNonCc=False)
    buildRegDataInst("ssub16", '''
            uint32_t geBits = 0;
            resTemp = 0;
            for (unsigned i = 0; i < 2; i++) {
                int high = (i + 1) * 16 - 1;
                int low = i * 16;
                int32_t midRes = sext<16>(bits(Op1_sw, high, low)) -
                                 sext<16>(bits(Op2_sw, high, low));
                replaceBits(resTemp, high, low, midRes);
                if (midRes >= 0) {
                    geBits = geBits | (0x3 << (i * 2));
                }
            }
            Dest = resTemp;
            resTemp = geBits;
        ''', flagType="ge", buildNonCc=False)
    buildRegDataInst("sasx", '''
            int32_t midRes, geBits = 0;
            resTemp = 0;
            int64_t arg1Low = sext<16>(bits(Op1_sw, 15, 0));
            int64_t arg1High = sext<16>(bits(Op1_sw, 31, 16));
            int64_t arg2Low = sext<16>(bits(Op2_sw, 15, 0));
            int64_t arg2High = sext<16>(bits(Op2_sw, 31, 16));
            midRes = arg1Low - arg2High;
            if (midRes >= 0) {
                geBits = geBits | 0x3;
            }
            replaceBits(resTemp, 15, 0, midRes);
            midRes = arg1High + arg2Low;
            if (midRes >= 0) {
                geBits = geBits | 0xc;
            }
            replaceBits(resTemp, 31, 16, midRes);
            Dest = resTemp;
            resTemp = geBits;
        ''', flagType="ge", buildNonCc=True)
    buildRegDataInst("ssax", '''
            int32_t midRes, geBits = 0;
            resTemp = 0;
            int64_t arg1Low = sext<16>(bits(Op1_sw, 15, 0));
            int64_t arg1High = sext<16>(bits(Op1_sw, 31, 16));
            int64_t arg2Low = sext<16>(bits(Op2_sw, 15, 0));
            int64_t arg2High = sext<16>(bits(Op2_sw, 31, 16));
            midRes = arg1Low + arg2High;
            if (midRes >= 0) {
                geBits = geBits | 0x3;
            }
            replaceBits(resTemp, 15, 0, midRes);
            midRes = arg1High - arg2Low;
            if (midRes >= 0) {
                geBits = geBits | 0xc;
            }
            replaceBits(resTemp, 31, 16, midRes);
            Dest = resTemp;
            resTemp = geBits;
        ''', flagType="ge", buildNonCc=True)

    buildRegDataInst("shadd8", '''
            resTemp = 0;
            for (unsigned i = 0; i < 4; i++) {
                int high = (i + 1) * 8 - 1;
                int low = i * 8;
                int32_t midRes =
                    (uint64_t)(sext<8>(bits(Op1_sw, high, low)) +
                               sext<8>(bits(Op2_sw, high, low))) >> 1;
                replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("shadd16", '''
            resTemp = 0;
            for (unsigned i = 0; i < 2; i++) {
                int high = (i + 1) * 16 - 1;
                int low = i * 16;
                int32_t midRes =
                    (uint64_t)(sext<16>(bits(Op1_sw, high, low)) +
                               sext<16>(bits(Op2_sw, high, low))) >> 1;
                replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("shsub8", '''
            resTemp = 0;
            for (unsigned i = 0; i < 4; i++) {
                int high = (i + 1) * 8 - 1;
                int low = i * 8;
                int32_t midRes =
                    (uint64_t)(sext<8>(bits(Op1_sw, high, low)) -
                               sext<8>(bits(Op2_sw, high, low))) >> 1;
                replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("shsub16", '''
            resTemp = 0;
            for (unsigned i = 0; i < 2; i++) {
                int high = (i + 1) * 16 - 1;
                int low = i * 16;
                int32_t midRes =
                    (uint64_t)(sext<16>(bits(Op1_sw, high, low)) -
                               sext<16>(bits(Op2_sw, high, low))) >> 1;
                replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("shasx", '''
            int32_t midRes;
            resTemp = 0;
            int64_t arg1Low = sext<16>(bits(Op1_sw, 15, 0));
            int64_t arg1High = sext<16>(bits(Op1_sw, 31, 16));
            int64_t arg2Low = sext<16>(bits(Op2_sw, 15, 0));
            int64_t arg2High = sext<16>(bits(Op2_sw, 31, 16));
            midRes = (uint64_t)(arg1Low - arg2High) >> 1;
            replaceBits(resTemp, 15, 0, midRes);
            midRes = (arg1High + arg2Low) >> 1;
            replaceBits(resTemp, 31, 16, midRes);
            Dest = resTemp;
        ''', flagType="none", buildCc=True)
    buildRegDataInst("shsax", '''
            int32_t midRes;
            resTemp = 0;
            int64_t arg1Low = sext<16>(bits(Op1_sw, 15, 0));
            int64_t arg1High = sext<16>(bits(Op1_sw, 31, 16));
            int64_t arg2Low = sext<16>(bits(Op2_sw, 15, 0));
            int64_t arg2High = sext<16>(bits(Op2_sw, 31, 16));
            midRes = (uint64_t)(arg1Low + arg2High) >> 1;
            replaceBits(resTemp, 15, 0, midRes);
            midRes = (uint64_t)(arg1High - arg2Low) >> 1;
            replaceBits(resTemp, 31, 16, midRes);
            Dest = resTemp;
        ''', flagType="none", buildCc=True)

    buildRegDataInst("uqadd16", '''
            uint32_t midRes;
            for (unsigned i = 0; i < 2; i++) {
                int high = (i + 1) * 16 - 1;
                int low = i * 16;
                uint64_t arg1 = bits(Op1, high, low);
                uint64_t arg2 = bits(Op2, high, low);
                uSaturateOp<16>(midRes, arg1, arg2);
                replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("uqadd8", '''
            uint32_t midRes;
            for (unsigned i = 0; i < 4; i++) {
                int high = (i + 1) * 8 - 1;
                int low = i * 8;
                uint64_t arg1 = bits(Op1, high, low);
                uint64_t arg2 = bits(Op2, high, low);
                uSaturateOp<8>(midRes, arg1, arg2);
                replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("uqsub16", '''
            uint32_t midRes;
            for (unsigned i = 0; i < 2; i++) {
                 int high = (i + 1) * 16 - 1;
                 int low = i * 16;
                 uint64_t arg1 = bits(Op1, high, low);
                 uint64_t arg2 = bits(Op2, high, low);
                 uSaturateOp<16>(midRes, arg1, arg2, true);
                 replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("uqsub8", '''
            uint32_t midRes;
            for (unsigned i = 0; i < 4; i++) {
                 int high = (i + 1) * 8 - 1;
                 int low = i * 8;
                 uint64_t arg1 = bits(Op1, high, low);
                 uint64_t arg2 = bits(Op2, high, low);
                 uSaturateOp<8>(midRes, arg1, arg2, true);
                 replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("uqasx", '''
            uint32_t midRes;
            uint64_t arg1Low = bits(Op1_sw, 15, 0);
            uint64_t arg1High = bits(Op1_sw, 31, 16);
            uint64_t arg2Low = bits(Op2_sw, 15, 0);
            uint64_t arg2High = bits(Op2_sw, 31, 16);
            uSaturateOp<16>(midRes, arg1Low, arg2High, true);
            replaceBits(resTemp, 15, 0, midRes);
            uSaturateOp<16>(midRes, arg1High, arg2Low);
            replaceBits(resTemp, 31, 16, midRes);
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("uqsax", '''
            uint32_t midRes;
            uint64_t arg1Low = bits(Op1_sw, 15, 0);
            uint64_t arg1High = bits(Op1_sw, 31, 16);
            uint64_t arg2Low = bits(Op2_sw, 15, 0);
            uint64_t arg2High = bits(Op2_sw, 31, 16);
            uSaturateOp<16>(midRes, arg1Low, arg2High);
            replaceBits(resTemp, 15, 0, midRes);
            uSaturateOp<16>(midRes, arg1High, arg2Low, true);
            replaceBits(resTemp, 31, 16, midRes);
            Dest = resTemp;
        ''', flagType="none", buildCc=False)

    buildRegDataInst("uadd16", '''
            uint32_t geBits = 0;
            resTemp = 0;
            for (unsigned i = 0; i < 2; i++) {
                int high = (i + 1) * 16 - 1;
                int low = i * 16;
                int32_t midRes = bits(Op1, high, low) +
                                 bits(Op2, high, low);
                if (midRes >= 0x10000) {
                    geBits = geBits | (0x3 << (i * 2));
                }
                replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
            resTemp = geBits;
        ''', flagType="ge", buildNonCc=False)
    buildRegDataInst("uadd8", '''
            uint32_t geBits = 0;
            resTemp = 0;
            for (unsigned i = 0; i < 4; i++) {
                int high = (i + 1) * 8 - 1;
                int low = i * 8;
                int32_t midRes = bits(Op1, high, low) +
                                 bits(Op2, high, low);
                if (midRes >= 0x100) {
                    geBits = geBits | (1 << i);
                }
                replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
            resTemp = geBits;
        ''', flagType="ge", buildNonCc=False)
    buildRegDataInst("usub16", '''
            uint32_t geBits = 0;
            resTemp = 0;
            for (unsigned i = 0; i < 2; i++) {
                int high = (i + 1) * 16 - 1;
                int low = i * 16;
                int32_t midRes = bits(Op1, high, low) -
                                 bits(Op2, high, low);
                if (midRes >= 0) {
                    geBits = geBits | (0x3 << (i * 2));
                }
                replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
            resTemp = geBits;
        ''', flagType="ge", buildNonCc=False)
    buildRegDataInst("usub8", '''
            uint32_t geBits = 0;
            resTemp = 0;
            for (unsigned i = 0; i < 4; i++) {
                int high = (i + 1) * 8 - 1;
                int low = i * 8;
                int32_t midRes = bits(Op1, high, low) -
                                 bits(Op2, high, low);
                if (midRes >= 0) {
                    geBits = geBits | (1 << i);
                }
                replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
            resTemp = geBits;
        ''', flagType="ge", buildNonCc=False)
    buildRegDataInst("uasx", '''
            int32_t midRes, geBits = 0;
            resTemp = 0;
            int64_t arg1Low = bits(Op1_sw, 15, 0);
            int64_t arg1High = bits(Op1_sw, 31, 16);
            int64_t arg2Low = bits(Op2_sw, 15, 0);
            int64_t arg2High = bits(Op2_sw, 31, 16);
            midRes = arg1Low - arg2High;
            if (midRes >= 0) {
                geBits = geBits | 0x3;
            }
            replaceBits(resTemp, 15, 0, midRes);
            midRes = arg1High + arg2Low;
            if (midRes >= 0x10000) {
                geBits = geBits | 0xc;
            }
            replaceBits(resTemp, 31, 16, midRes);
            Dest = resTemp;
            resTemp = geBits;
        ''', flagType="ge", buildNonCc=False)
    buildRegDataInst("usax", '''
            int32_t midRes, geBits = 0;
            resTemp = 0;
            int64_t arg1Low = bits(Op1_sw, 15, 0);
            int64_t arg1High = bits(Op1_sw, 31, 16);
            int64_t arg2Low = bits(Op2_sw, 15, 0);
            int64_t arg2High = bits(Op2_sw, 31, 16);
            midRes = arg1Low + arg2High;
            if (midRes >= 0x10000) {
                geBits = geBits | 0x3;
            }
            replaceBits(resTemp, 15, 0, midRes);
            midRes = arg1High - arg2Low;
            if (midRes >= 0) {
                geBits = geBits | 0xc;
            }
            replaceBits(resTemp, 31, 16, midRes);
            Dest = resTemp;
            resTemp = geBits;
        ''', flagType="ge", buildNonCc=False)

    buildRegDataInst("uhadd16", '''
            resTemp = 0;
            for (unsigned i = 0; i < 2; i++) {
                int high = (i + 1) * 16 - 1;
                int low = i * 16;
                int32_t midRes = (bits(Op1, high, low) +
                                  bits(Op2, high, low)) >> 1;
                replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("uhadd8", '''
            resTemp = 0;
            for (unsigned i = 0; i < 4; i++) {
                int high = (i + 1) * 8 - 1;
                int low = i * 8;
                int32_t midRes = (bits(Op1, high, low) +
                                  bits(Op2, high, low)) >> 1;
                replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("uhsub16", '''
            resTemp = 0;
            for (unsigned i = 0; i < 2; i++) {
                int high = (i + 1) * 16 - 1;
                int low = i * 16;
                int32_t midRes = (bits(Op1, high, low) -
                                  bits(Op2, high, low)) >> 1;
                replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("uhsub8", '''
            resTemp = 0;
            for (unsigned i = 0; i < 4; i++) {
                int high = (i + 1) * 8 - 1;
                int low = i * 8;
                int32_t midRes = (bits(Op1, high, low) -
                                  bits(Op2, high, low)) >> 1;
                replaceBits(resTemp, high, low, midRes);
            }
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("uhasx", '''
            int32_t midRes;
            resTemp = 0;
            int64_t arg1Low = bits(Op1_sw, 15, 0);
            int64_t arg1High = bits(Op1_sw, 31, 16);
            int64_t arg2Low = bits(Op2_sw, 15, 0);
            int64_t arg2High = bits(Op2_sw, 31, 16);
            midRes = (arg1Low - arg2High) >> 1;
            replaceBits(resTemp, 15, 0, midRes);
            midRes = (arg1High + arg2Low) >> 1;
            replaceBits(resTemp, 31, 16, midRes);
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("uhsax", '''
            int32_t midRes;
            resTemp = 0;
            int64_t arg1Low = bits(Op1_sw, 15, 0);
            int64_t arg1High = bits(Op1_sw, 31, 16);
            int64_t arg2Low = bits(Op2_sw, 15, 0);
            int64_t arg2High = bits(Op2_sw, 31, 16);
            midRes = (arg1Low + arg2High) >> 1;
            replaceBits(resTemp, 15, 0, midRes);
            midRes = (arg1High - arg2Low) >> 1;
            replaceBits(resTemp, 31, 16, midRes);
            Dest = resTemp;
        ''', flagType="none", buildCc=False)

    buildRegDataInst("pkhbt", '''
            uint32_t resTemp = 0;
            uint16_t arg1Low = bits(Op1, 15, 0);
            uint16_t arg2High = bits(secondOp, 31, 16);
            replaceBits(resTemp, 15, 0, arg1Low);
            replaceBits(resTemp, 31, 16, arg2High);
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
    buildRegDataInst("pkhtb", '''
            uint32_t resTemp = 0;
            uint16_t arg1High = bits(Op1, 31, 16);
            uint16_t arg2Low = bits(secondOp, 15, 0);
            replaceBits(resTemp, 15, 0, arg2Low);
            replaceBits(resTemp, 31, 16, arg1High);
            Dest = resTemp;
        ''', flagType="none", buildCc=False)
}};
