# configuration file generated by Bochs
plugin_ctrl: unmapped=1, biosdev=1, speaker=1, extfpuirq=1, pci_ide=1, acpi=1, ioapic=1
config_interface: textconfig
display_library: x
memory: host=32, guest=32
romimage: file="/usr/share/bochs/BIOS-bochs-latest"
vgaromimage: file="/usr/share/bochs/VGABIOS-lgpl-latest"
boot: cdrom
floppy_bootsig_check: disabled=0
floppya: type=1_44, 1_44="a.img", status=inserted, write_protected=0
# no floppyb
ata0: enabled=1, ioaddr1=0x1f0, ioaddr2=0x3f0, irq=14
ata1: enabled=1, ioaddr1=0x170, ioaddr2=0x370, irq=15
ata2: enabled=0
ata3: enabled=0
ata0-slave: type=cdrom, path=fli4l.iso, status=inserted
parport1: enabled=1, file=""
parport2: enabled=0
com1: enabled=1, mode=null, dev=""
com2: enabled=0
com3: enabled=0
com4: enabled=0
usb_uhci: enabled=0
usb_ohci: enabled=0
i440fxsupport: enabled=1
vga_update_interval: 50000
vga: extension=vbe
cpu: count=1, ips=4000000, reset_on_triple_fault=1, ignore_bad_msrs=1
cpuid: cpuid_limit_winnt=0, mmx=1, sse=sse2, xapic=1, sep=1, aes=0, xsave=0, movbe=0
cpuid: stepping=3, vendor_string="GenuineIntel", brand_string="              Intel(R) Pentium(R) 4 CPU        "
print_timestamps: enabled=0
# no gdb stub
port_e9_hack: enabled=0
text_snapshot_check: enabled=0
private_colormap: enabled=0
clock: sync=none, time0=local
# no cmosimage
ne2k: card=0, enabled=1, ioaddr=0x320, irq=10, mac=fe:fd:00:00:00:02, ethmod=tuntap, ethdev=/dev/net/tun:tap0, script=none
ne2k: card=1, enabled=0, ioaddr=0x320, irq=7, mac=fe:fd:00:00:00:01, ethmod=null, ethdev=xl0, script=none
ne2k: card=2, enabled=0
ne2k: card=3, enabled=0
pnic: enabled=0
sb16: enabled=0
# no loader
log: -
logprefix: %t%e%d
panic: action=ask
error: action=report
info: action=report
debug: action=ignore
pass: action=fatal
keyboard_type: mf
keyboard_serial_delay: 250
keyboard_paste_delay: 100000
keyboard_mapping: enabled=0, map=
user_shortcut: keys=none
mouse: enabled=0, type=ps2, toggle=ctrl+mbutton
