// Copyright (c) 2006-2007 The Regents of The University of Michigan
// All rights reserved.
//
// Redistribution and use in source and binary forms, with or without
// modification, are permitted provided that the following conditions are
// met: redistributions of source code must retain the above copyright
// notice, this list of conditions and the following disclaimer;
// redistributions in binary form must reproduce the above copyright
// notice, this list of conditions and the following disclaimer in the
// documentation and/or other materials provided with the distribution;
// neither the name of the copyright holders nor the names of its
// contributors may be used to endorse or promote products derived from
// this software without specific prior written permission.
//
// THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
// "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
// LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
// A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
// OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
// SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
// LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
// DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
// THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
// (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
// OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
//
// Authors: Ali Saidi
//          Gabe Black
//          Steve Reinhardt

def operand_types {{
    'sb' : 'int8_t',
    'ub' : 'uint8_t',
    'shw' : 'int16_t',
    'uhw' : 'uint16_t',
    'sw' : 'int32_t',
    'uw' : 'uint32_t',
    'sdw' : 'int64_t',
    'udw' : 'uint64_t',
    'tudw' : 'Twin64_t',
    'tuw' : 'Twin32_t',
    'sf' : 'float',
    'df' : 'double',

    'pstate' : 'PSTATE',
    'hpstate' : 'HPSTATE'
}};

output header {{
    // A function to "decompress" double and quad floating point
    // register numbers stuffed into 5 bit fields. These have their
    // MSB put in the LSB position but are otherwise normal.
    static inline unsigned int
    dfpr(unsigned int regNum)
    {
        return (regNum & (~1)) | ((regNum & 1) << 5);
    }

    static inline unsigned int
    dfprl(unsigned int regNum)
    {
        return dfpr(regNum) & (~0x1);
    }

    static inline unsigned int
    dfprh(unsigned int regNum)
    {
        return dfpr(regNum) | 0x1;
    }
}};

def operands {{
    # Int regs default to unsigned, but code should not count on this.
    # For clarity, descriptions that depend on unsigned behavior should
    # explicitly specify '.uq'.

    'Rd':               ('IntReg', 'udw', 'RD', 'IsInteger', 1),
    # The Rd from the previous window
    'Rd_prev':          ('IntReg', 'udw', 'RD + NumIntArchRegs + NumMicroIntRegs', 'IsInteger', 2),
    # The Rd from the next window
    'Rd_next':          ('IntReg', 'udw', 'RD + 2 * NumIntArchRegs + NumMicroIntRegs', 'IsInteger', 3),
    # For microcoded twin load instructions, RdTwin appears in the "code"
    # for the instruction is replaced by RdLow or RdHigh by the format
    # before it's processed by the iop.
    # The low (even) register of a two register pair
    'RdLow':            ('IntReg', 'udw', 'RD & (~1)', 'IsInteger', 4),
    # The high (odd) register of a two register pair
    'RdHigh':           ('IntReg', 'udw', 'RD | 1', 'IsInteger', 5),
    'Rs1':              ('IntReg', 'udw', 'RS1', 'IsInteger', 6),
    'Rs2':              ('IntReg', 'udw', 'RS2', 'IsInteger', 7),
    # A microcode register. Right now, this is the only one.
    'uReg0':            ('IntReg', 'udw', 'NumIntArchRegs', 'IsInteger', 8),
    # Because double and quad precision register numbers are decoded
    # differently, they get different operands. The single precision versions
    # have an s post pended to their name.
    'Frds':             ('FloatReg', 'sf', 'RD', 'IsFloating', 10),
    #'Frd':             ('FloatReg', 'df', 'dfpr(RD)', 'IsFloating', 10),
    'Frd_low':          ('FloatReg', 'uw', 'dfprl(RD)', 'IsFloating', 10),
    'Frd_high':         ('FloatReg', 'uw', 'dfprh(RD)', 'IsFloating', 10),
    # Each Frd_N refers to the Nth double precision register from Frd.
    # Note that this adds twice N to the register number.
    #'Frd_0':           ('FloatReg', 'df', 'dfpr(RD)', 'IsFloating', 10),
    'Frd_0_low':        ('FloatReg', 'uw', 'dfprl(RD)', 'IsFloating', 10),
    'Frd_0_high':       ('FloatReg', 'uw', 'dfprh(RD)', 'IsFloating', 10),
    #'Frd_1':           ('FloatReg', 'df', 'dfpr(RD) + 2', 'IsFloating', 10),
    'Frd_1_low':        ('FloatReg', 'uw', 'dfprl(RD) + 2', 'IsFloating', 10),
    'Frd_1_high':       ('FloatReg', 'uw', 'dfprh(RD) + 2', 'IsFloating', 10),
    #'Frd_2':           ('FloatReg', 'df', 'dfpr(RD) + 4', 'IsFloating', 10),
    'Frd_2_low':        ('FloatReg', 'uw', 'dfprl(RD) + 4', 'IsFloating', 10),
    'Frd_2_high':       ('FloatReg', 'uw', 'dfprh(RD) + 4', 'IsFloating', 10),
    #'Frd_3':           ('FloatReg', 'df', 'dfpr(RD) + 6', 'IsFloating', 10),
    'Frd_3_low':        ('FloatReg', 'uw', 'dfprl(RD) + 6', 'IsFloating', 10),
    'Frd_3_high':       ('FloatReg', 'uw', 'dfprh(RD) + 6', 'IsFloating', 10),
    #'Frd_4':           ('FloatReg', 'df', 'dfpr(RD) + 8', 'IsFloating', 10),
    'Frd_4_low':        ('FloatReg', 'uw', 'dfprl(RD) + 8', 'IsFloating', 10),
    'Frd_4_high':       ('FloatReg', 'uw', 'dfprh(RD) + 8', 'IsFloating', 10),
    #'Frd_5':           ('FloatReg', 'df', 'dfpr(RD) + 10', 'IsFloating', 10),
    'Frd_5_low':        ('FloatReg', 'uw', 'dfprl(RD) + 10', 'IsFloating', 10),
    'Frd_5_high':       ('FloatReg', 'uw', 'dfprh(RD) + 10', 'IsFloating', 10),
    #'Frd_6':           ('FloatReg', 'df', 'dfpr(RD) + 12', 'IsFloating', 10),
    'Frd_6_low':        ('FloatReg', 'uw', 'dfprl(RD) + 12', 'IsFloating', 10),
    'Frd_6_high':       ('FloatReg', 'uw', 'dfprh(RD) + 12', 'IsFloating', 10),
    #'Frd_7':           ('FloatReg', 'df', 'dfpr(RD) + 14', 'IsFloating', 10),
    'Frd_7_low':        ('FloatReg', 'uw', 'dfprl(RD) + 14', 'IsFloating', 10),
    'Frd_7_high':       ('FloatReg', 'uw', 'dfprh(RD) + 14', 'IsFloating', 10),
    'Frs1s':            ('FloatReg', 'sf', 'RS1', 'IsFloating', 11),
    #'Frs1':            ('FloatReg', 'df', 'dfpr(RS1)', 'IsFloating', 11),
    'Frs1_low':         ('FloatReg', 'uw', 'dfprl(RS1)', 'IsFloating', 11),
    'Frs1_high':        ('FloatReg', 'uw', 'dfprh(RS1)', 'IsFloating', 11),
    'Frs2s':            ('FloatReg', 'sf', 'RS2', 'IsFloating', 12),
    #'Frs2':            ('FloatReg', 'df', 'dfpr(RS2)', 'IsFloating', 12),
    'Frs2_low':         ('FloatReg', 'uw', 'dfprl(RS2)', 'IsFloating', 12),
    'Frs2_high':        ('FloatReg', 'uw', 'dfprh(RS2)', 'IsFloating', 12),
    'PC':               ('PCState', 'udw', 'pc', (None, None, 'IsControl'), 30),
    'NPC':              ('PCState', 'udw', 'npc', (None, None, 'IsControl'), 30),
    'NNPC':             ('PCState', 'udw', 'nnpc', (None, None, 'IsControl'), 30),
    # Registers which are used explicitly in instructions
    'R0':               ('IntReg', 'udw', '0', None, 6),
    'R1':               ('IntReg', 'udw', '1', None, 7),
    'R15':              ('IntReg', 'udw', '15', 'IsInteger', 8),
    'R16':              ('IntReg', 'udw', '16', None, 9),
    'O0':               ('IntReg', 'udw', '8', 'IsInteger', 10),
    'O1':               ('IntReg', 'udw', '9', 'IsInteger', 11),
    'O2':               ('IntReg', 'udw', '10', 'IsInteger', 12),
    'O3':               ('IntReg', 'udw', '11', 'IsInteger', 13),
    'O4':               ('IntReg', 'udw', '12', 'IsInteger', 14),
    'O5':               ('IntReg', 'udw', '13', 'IsInteger', 15),

    # Control registers
#   'Y':                ('ControlReg', 'udw', 'MISCREG_Y', None, 40),
#   'Ccr':              ('ControlReg', 'udw', 'MISCREG_CCR', None, 41),
    'Y':                ('IntReg', 'udw', 'NumIntArchRegs + 1', None, 40),
    'Ccr':              ('IntReg', 'udw', 'NumIntArchRegs + 2', None, 41),
    'Asi':              ('ControlReg', 'udw', 'MISCREG_ASI', None, 42),
    'Fprs':             ('ControlReg', 'udw', 'MISCREG_FPRS', None, 43),
    'Pcr':              ('ControlReg', 'udw', 'MISCREG_PCR', None, 44),
    'Pic':              ('ControlReg', 'udw', 'MISCREG_PIC', None, 45),
#   'Gsr':              ('ControlReg', 'udw', 'MISCREG_GSR', (None, None, ['IsSerializeAfter','IsSerializing','IsNonSpeculative']), 46),
    'Gsr':              ('IntReg', 'udw', 'NumIntArchRegs + 8', None, 46),
    'Softint':          ('ControlReg', 'udw', 'MISCREG_SOFTINT', None, 47),
    'SoftintSet':       ('ControlReg', 'udw', 'MISCREG_SOFTINT_SET', None, 48),
    'SoftintClr':       ('ControlReg', 'udw', 'MISCREG_SOFTINT_CLR', None, 49),
    'TickCmpr':         ('ControlReg', 'udw', 'MISCREG_TICK_CMPR', None, 50),
    'Stick':            ('ControlReg', 'udw', 'MISCREG_STICK', None, 51),
    'StickCmpr':        ('ControlReg', 'udw', 'MISCREG_STICK_CMPR', None, 52),

    'Tpc':              ('ControlReg', 'udw', 'MISCREG_TPC', None, 53),
    'Tnpc':             ('ControlReg', 'udw', 'MISCREG_TNPC', None, 54),
    'Tstate':           ('ControlReg', 'udw', 'MISCREG_TSTATE', None, 55),
    'Tt':               ('ControlReg', 'udw', 'MISCREG_TT', None, 56),
    'Tick':             ('ControlReg', 'udw', 'MISCREG_TICK', None, 57),
    'Tba':              ('ControlReg', 'udw', 'MISCREG_TBA', None, 58),
    'Pstate':           ('ControlReg', 'pstate', 'MISCREG_PSTATE', None, 59),
    'Tl':               ('ControlReg', 'udw', 'MISCREG_TL', None, 60),
    'Pil':              ('ControlReg', 'udw', 'MISCREG_PIL', None, 61),
    'Cwp':              ('ControlReg', 'udw', 'MISCREG_CWP', (None, None, ['IsSerializeAfter','IsSerializing','IsNonSpeculative']), 62),
#   'Cansave':          ('ControlReg', 'udw', 'MISCREG_CANSAVE', None, 63),
#   'Canrestore':       ('ControlReg', 'udw', 'MISCREG_CANRESTORE', None, 64),
#   'Cleanwin':         ('ControlReg', 'udw', 'MISCREG_CLEANWIN', None, 65),
#   'Otherwin':         ('ControlReg', 'udw', 'MISCREG_OTHERWIN', None, 66),
#   'Wstate':           ('ControlReg', 'udw', 'MISCREG_WSTATE', None, 67),
    'Cansave':          ('IntReg', 'udw', 'NumIntArchRegs + 3', None, 63),
    'Canrestore':       ('IntReg', 'udw', 'NumIntArchRegs + 4', None, 64),
    'Cleanwin':         ('IntReg', 'udw', 'NumIntArchRegs + 5', None, 65),
    'Otherwin':         ('IntReg', 'udw', 'NumIntArchRegs + 6', None, 66),
    'Wstate':           ('IntReg', 'udw', 'NumIntArchRegs + 7', None, 67),
    'Gl':               ('ControlReg', 'udw', 'MISCREG_GL', None, 68),

    'Hpstate':          ('ControlReg', 'hpstate', 'MISCREG_HPSTATE', None, 69),
    'Htstate':          ('ControlReg', 'udw', 'MISCREG_HTSTATE', None, 70),
    'Hintp':            ('ControlReg', 'udw', 'MISCREG_HINTP', None, 71),
    'Htba':             ('ControlReg', 'udw', 'MISCREG_HTBA', None, 72),
    'HstickCmpr':       ('ControlReg', 'udw', 'MISCREG_HSTICK_CMPR', None, 73),
    'Hver':             ('ControlReg', 'udw', 'MISCREG_HVER', None, 74),
    'StrandStsReg':     ('ControlReg', 'udw', 'MISCREG_STRAND_STS_REG', None, 75),

    'Fsr':              ('ControlReg', 'udw', 'MISCREG_FSR', (None, None, ['IsSerializeAfter','IsSerializing','IsNonSpeculative']), 80),
    # Mem gets a large number so it's always last
    'Mem':              ('Mem', 'udw', None, ('IsMemRef', 'IsLoad', 'IsStore'), 100)

}};
