// -*- mode:c++ -*-

// Copyright (c) 2007 MIPS Technologies, Inc.
// All rights reserved.
//
// Redistribution and use in source and binary forms, with or without
// modification, are permitted provided that the following conditions are
// met: redistributions of source code must retain the above copyright
// notice, this list of conditions and the following disclaimer;
// redistributions in binary form must reproduce the above copyright
// notice, this list of conditions and the following disclaimer in the
// documentation and/or other materials provided with the distribution;
// neither the name of the copyright holders nor the names of its
// contributors may be used to endorse or promote products derived from
// this software without specific prior written permission.
//
// THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
// "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
// LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
// A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
// OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
// SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
// LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
// DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
// THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
// (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
// OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
//
// Authors: Korey Sewell
//          Brett Miller

////////////////////////////////////////////////////////////////////
//
// DSP integer operate instructions
//
output header {{
#include <iostream>
    using namespace std;
    /**
     * Base class for integer operations.
     */
    class DspIntOp : public MipsStaticInst
    {
      protected:

        /// Constructor
        DspIntOp(const char *mnem, MachInst _machInst, OpClass __opClass) :
            MipsStaticInst(mnem, _machInst, __opClass)
        {
        }
    };

    class DspHiLoOp : public MipsStaticInst
    {
      protected:

        /// Constructor
        DspHiLoOp(const char *mnem, MachInst _machInst, OpClass __opClass) :
            MipsStaticInst(mnem, _machInst, __opClass)
        {
        }
    };
}};

// Dsp instruction class execute method template.
def template DspExecute {{
        Fault %(class_name)s::execute(%(CPU_exec_context)s *xc, Trace::InstRecord *traceData) const
        {
                Fault fault = NoFault;

                %(op_decl)s;

                if (isDspPresent(xc))
                {
                    if (isDspEnabled(xc))
                    {
                        %(op_rd)s;
                        %(code)s;
                    }
                    else
                    {
                        fault = new DspStateDisabledFault();
                    }
                }
                else
                {
                    fault = new ReservedInstructionFault();
                }

                if(fault == NoFault)
                {
                    %(op_wb)s;
                }
                return fault;
        }
}};

// DspHiLo instruction class execute method template.
def template DspHiLoExecute {{
        Fault %(class_name)s::execute(%(CPU_exec_context)s *xc, Trace::InstRecord *traceData) const
        {
                Fault fault = NoFault;

                %(op_decl)s;

                if (isDspPresent(xc))
                {
                    if (isDspEnabled(xc))
                    {
                        %(op_rd)s;
                        %(code)s;
                    }
                    else
                    {
                        fault = new DspStateDisabledFault();
                    }
                }
                else
                {
                    fault = new ReservedInstructionFault();
                }

                if(fault == NoFault)
                {
                    %(op_wb)s;
                    //If there are 2 Destination Registers then
                    //concatenate the values for the traceData
                    if(traceData && _numDestRegs == 2) {
                        // FIXME - set the trace value correctly here
                        //uint64_t hilo_final_val = (uint64_t)HI_RD_SEL << 32 | LO_RD_SEL;
                        //traceData->setData(hilo_final_val);
                    }
                }
                return fault;
        }
}};

//Outputs to decoder.cc
output decoder {{
}};

output exec {{
    bool
    isDspEnabled(%(CPU_exec_context)s *xc)
    {
        return !FullSystem || bits(xc->readMiscReg(MISCREG_STATUS), 24);
    }
}};

output exec {{
    bool
    isDspPresent(%(CPU_exec_context)s *xc)
    {
        return !FullSystem || bits(xc->readMiscReg(MISCREG_CONFIG3), 10);
    }
}};

// add code to fetch the DSPControl register
// and write it back after execution, giving
// the instruction the opportunity to modify
// it if necessary
def format DspIntOp(code, *opt_flags) {{

    decl_code = 'uint32_t dspctl;\n'
    decl_code += 'dspctl = DSPControl;\n'

    write_code = 'DSPControl = dspctl;\n'

    code = decl_code + code + write_code

    opt_flags += ('IsDspOp',)

    iop = InstObjParams(name, Name, 'DspIntOp', code, opt_flags)
    header_output = BasicDeclare.subst(iop)
    decoder_output = BasicConstructor.subst(iop)
    decode_block = BasicDecode.subst(iop)
    exec_output = DspExecute.subst(iop)
}};

// add code to fetch the DSPControl register
// and write it back after execution, giving
// the instruction the opportunity to modify
// it if necessary; also, fetch the appropriate
// HI/LO register pair, based on the AC
// instruction field.

def format DspHiLoOp(code, *opt_flags) {{

    decl_code = 'int64_t dspac;\n'
    decl_code += 'uint32_t dspctl;\n'

    fetch_code = 'dspctl = DSPControl;\n'
    fetch_code += 'dspac = HI_RD_SEL;\n'
    fetch_code += 'dspac = dspac << 32 | LO_RD_SEL;\n'

    write_code = 'DSPControl = dspctl;\n'
    write_code += 'HI_RD_SEL = dspac<63:32>;\n'
    write_code += 'LO_RD_SEL = dspac<31:0>;\n'

    code = decl_code + fetch_code + code + write_code

    opt_flags += ('IsDspOp',)

    iop = InstObjParams(name, Name, 'DspHiLoOp', code, opt_flags)
    header_output = BasicDeclare.subst(iop)
    decoder_output = BasicConstructor.subst(iop)
    decode_block = BasicDecode.subst(iop)
    exec_output = DspHiLoExecute.subst(iop)

}};



